(footprint "VSSOP-8_3.0x3.0mm_P0.65mm-0.08space" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf")
  (tags "VSSOP-8 3.0 x 3.0")
  (property "Sheetfile" "headamp.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Single 40 μA Micropower Instrumentation Amplifier with Zero Crossover Distortion, MSOP-8")
  (property "ki_keywords" "single instumentation amplifier")
  (attr smd)
  (fp_text reference "U1" (at 0 -2.5) (layer "F.SilkS"))
  (fp_text value "IN849" (at 0.02 2.73) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
  (pad "1" smd rect (at -2.2 -0.975 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -2.2 -0.325 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -2.2 0.325 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -2.2 0.975 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 2.2 0.975 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 2.2 0.325 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 2.2 -0.325 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 2.2 -0.975 270) (size 0.4445 1.524) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/VSSOP-8_3.0x3.0mm_P0.65mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
