(kicad_pcb (version 4) (host pcbnew "(after 2015-mar-04 BZR unknown)-product")
  (general
    (links 224)
    (no_connects 0)
    (area 72.339999 23.063999 131.953001 167.944001)
    (thickness 1.6)
    (drawings 36)
    (tracks 468)
    (zones 0)
    (modules 26)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.508)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 9.398)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.020000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C2-Pad1)")
  (net 2 "Net-(P1-Pad1)")
  (net 3 "Net-(P1-Pad13)")
  (net 4 "Net-(P1-Pad14)")
  (net 5 "Net-(P1-Pad17)")
  (net 6 "Net-(P1-Pad18)")
  (net 7 "Net-(P5-Pad2)")
  (net 8 "Net-(P10-Pad2)")
  (net 9 "Net-(P10-Pad8)")
  (net 10 "Net-(P10-Pad14)")
  (net 11 "Net-(P10-Pad18)")
  (net 12 "Net-(P10-Pad20)")
  (net 13 "Net-(P10-Pad22)")
  (net 14 "Net-(P10-Pad26)")
  (net 15 "Net-(P10-Pad28)")
  (net 16 "Net-(P10-Pad30)")
  (net 17 "Net-(P10-Pad32)")
  (net 18 "Net-(P10-Pad34)")
  (net 19 "Net-(P10-Pad24)")
  (net 20 "Net-(P10-Pad6)")
  (net 21 "Net-(P10-Pad10)")
  (net 22 "Net-(P10-Pad12)")
  (net 23 GND)
  (net 24 +5V)
  (net 25 /24V)
  (net 26 "Net-(P2-Pad13)")
  (net 27 "Net-(P2-Pad14)")
  (net 28 "Net-(P2-Pad17)")
  (net 29 "Net-(P2-Pad18)")
  (net 30 "Net-(P2-Pad9)")
  (net 31 "Net-(P2-Pad10)")
  (net 32 "Net-(P10-Pad4)")
  (net 33 "Net-(C5-Pad2)")
  (net 34 "Net-(C6-Pad2)")
  (net 35 "Net-(U1-Pad4)")
  (net 36 "Net-(C1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P10-Pad10)")
    (add_net "Net-(P10-Pad12)")
    (add_net "Net-(P10-Pad14)")
    (add_net "Net-(P10-Pad18)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P10-Pad20)")
    (add_net "Net-(P10-Pad22)")
    (add_net "Net-(P10-Pad24)")
    (add_net "Net-(P10-Pad26)")
    (add_net "Net-(P10-Pad28)")
    (add_net "Net-(P10-Pad30)")
    (add_net "Net-(P10-Pad32)")
    (add_net "Net-(P10-Pad34)")
    (add_net "Net-(P10-Pad4)")
    (add_net "Net-(P10-Pad6)")
    (add_net "Net-(P10-Pad8)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad13)")
    (add_net "Net-(P2-Pad14)")
    (add_net "Net-(P2-Pad17)")
    (add_net "Net-(P2-Pad18)")
    (add_net "Net-(P2-Pad9)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(U1-Pad4)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /24V)
    (add_net GND)
  )
  (module econ20 (layer F.Cu) (tedit 615872BA)
    (at 125.476 117.373 90)
    (fp_text reference P1 (at -0.381 -6.35 90) (layer F.SilkS))
    (fp_text value CON20_SA1000 (at -5.08 0 90) (layer F.SilkS) hide)
    (fp_text user 19 (at -12.7 -6.477 90) (layer F.SilkS))
    (fp_text user 1 (at 9.906 -6.477 90) (layer F.SilkS))
    (pad 1 connect rect (at 10.0584 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 2 "Net-(P1-Pad1)") (solder_mask_margin 0.5334))
    (pad 2 connect rect (at 10.0584 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 3 connect rect (at 7.5184 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5334))
    (pad 4 connect rect (at 7.5184 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 5 connect rect (at 4.9784 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5334))
    (pad 6 connect rect (at 4.9784 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 7 connect rect (at 2.4384 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5334))
    (pad 8 connect rect (at 2.4384 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 9 connect rect (at -0.1016 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 10 connect rect (at -0.1016 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 11 connect rect (at -2.6416 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5334))
    (pad 12 connect rect (at -2.6416 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 13 connect rect (at -5.1816 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 3 "Net-(P1-Pad13)") (solder_mask_margin 0.5334))
    (pad 14 connect rect (at -5.1816 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 4 "Net-(P1-Pad14)") (solder_mask_margin 0.5334))
    (pad 15 connect rect (at -7.7216 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 16 connect rect (at -7.7216 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 17 connect rect (at -10.2616 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 5 "Net-(P1-Pad17)") (solder_mask_margin 0.5334))
    (pad 18 connect rect (at -10.2616 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 6 "Net-(P1-Pad18)") (solder_mask_margin 0.5334))
    (pad 19 connect rect (at -12.8016 -0.127 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 20 connect rect (at -12.8016 -0.127 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
  )
  (module ECON50 (layer F.Cu) (tedit 61587246)
    (at 119.38 49.4792 90)
    (fp_text reference P8 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value CON50 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user 49 (at -41.6052 -0.6604 90) (layer F.SilkS))
    (fp_text user 1 (at 18.8468 -0.7112 90) (layer F.SilkS))
    (pad 1 connect rect (at 18.9992 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 2 connect rect (at 18.9992 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 8 "Net-(P10-Pad2)") (solder_mask_margin 0.5334))
    (pad 3 connect rect (at 16.4592 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 4 connect rect (at 16.4592 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 32 "Net-(P10-Pad4)") (solder_mask_margin 0.5334))
    (pad 5 connect rect (at 13.9192 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 6 connect rect (at 13.9192 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 7 connect rect (at 11.3792 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 8 connect rect (at 11.3792 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 9 "Net-(P10-Pad8)") (solder_mask_margin 0.5334))
    (pad 9 connect rect (at 8.8392 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 10 connect rect (at 8.8392 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 11 connect rect (at 6.2992 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 12 connect rect (at 6.2992 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 13 connect rect (at 3.7592 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 14 connect rect (at 3.7592 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 10 "Net-(P10-Pad14)") (solder_mask_margin 0.5334))
    (pad 15 connect rect (at 1.2192 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 16 connect rect (at 1.2192 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 17 connect rect (at -1.3208 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 18 connect rect (at -1.3208 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 11 "Net-(P10-Pad18)") (solder_mask_margin 0.5334))
    (pad 19 connect rect (at -3.8608 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 20 connect rect (at -3.8608 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 12 "Net-(P10-Pad20)") (solder_mask_margin 0.5334))
    (pad 21 connect rect (at -6.4008 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 22 connect rect (at -6.4008 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 13 "Net-(P10-Pad22)") (solder_mask_margin 0.5334))
    (pad 23 connect rect (at -8.9408 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 24 connect rect (at -8.9408 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 25 connect rect (at -11.4808 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 26 connect rect (at -11.4808 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 14 "Net-(P10-Pad26)") (solder_mask_margin 0.5334))
    (pad 27 connect rect (at -14.0208 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 28 connect rect (at -14.0208 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 15 "Net-(P10-Pad28)") (solder_mask_margin 0.5334))
    (pad 29 connect rect (at -16.5608 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 30 connect rect (at -16.5608 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 16 "Net-(P10-Pad30)") (solder_mask_margin 0.5334))
    (pad 31 connect rect (at -19.1008 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 32 connect rect (at -19.1008 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 17 "Net-(P10-Pad32)") (solder_mask_margin 0.5334))
    (pad 33 connect rect (at -21.6408 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 34 connect rect (at -21.6408 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 18 "Net-(P10-Pad34)") (solder_mask_margin 0.5334))
    (pad 35 connect rect (at -24.1808 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 37 connect rect (at -26.7208 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 39 connect rect (at -29.2608 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 41 connect rect (at -31.8008 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 43 connect rect (at -34.3408 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 45 connect rect (at -36.8808 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 47 connect rect (at -39.4208 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 49 connect rect (at -41.9608 5.969 270) (size 1.524 9.398) (layers F.Cu F.Mask)
      (net 23 GND) (solder_mask_margin 0.5334))
    (pad 36 connect rect (at -24.1808 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 19 "Net-(P10-Pad24)") (solder_mask_margin 0.5334))
    (pad 38 connect rect (at -26.7208 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 40 connect rect (at -29.2608 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 20 "Net-(P10-Pad6)") (solder_mask_margin 0.5334))
    (pad 42 connect rect (at -31.8008 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 21 "Net-(P10-Pad10)") (solder_mask_margin 0.5334))
    (pad 44 connect rect (at -34.3408 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (net 22 "Net-(P10-Pad12)") (solder_mask_margin 0.5334))
    (pad 46 connect rect (at -36.8808 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 48 connect rect (at -39.4208 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
    (pad 50 connect rect (at -41.9608 5.969 270) (size 1.524 9.398) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5334))
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 61397925)
    (at 102.108 151.384)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C1 (at 7.62 -7.874) (layer F.SilkS))
    (fp_text value 10uf (at 0 3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C1-Pad2)"))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 6139791F)
    (at 109.22 148.844 90)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C2 (at -2.54 -13.462 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:DRVPWR (layer B.Cu) (tedit 0)
    (at 109.22 152.4 90)
    (fp_text reference P4 (at -5.715 1.905 90) (layer B.SilkS))
    (fp_text value CONN_4 (at -1.27 10.16 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at 6.35 5.08 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask B.SilkS)
      (net 1 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 5.08 90) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 3 thru_hole circle (at -3.81 5.08 90) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 4 thru_hole circle (at -8.89 5.08 90) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask B.SilkS)
      (net 24 +5V))
    (pad "" np_thru_hole circle (at -6.35 15.24 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 3.81 15.24 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -11.43 7.62 90) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 8.89 7.62 90) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask B.SilkS))
    (model /home/djg/mfm/all_fp.pretty/DRVPWR.wrl
      (at (xyz -0.05 0.21 0.185))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz -90 0 180))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 61395AE2)
    (at 101.346 123.444 90)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C3 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value .1uf (at -1.016 3.048 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 +5V))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Socket_Straight_2x10_Pitch2.54mm locked (layer F.Cu) (tedit 61395948)
    (at 78.74 82.55)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference P7 (at -1.524 -3.048) (layer F.SilkS))
    (fp_text value CON20 (at -1.27 25.19) (layer F.Fab))
    (fp_text user %R (at -1.27 11.43 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -2.54 2.54 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2.54 5.08 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -2.54 7.62 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.54 10.16 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 12.7 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 26 "Net-(P2-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 15.24 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 16 thru_hole oval (at -2.54 17.78 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 28 "Net-(P2-Pad17)"))
    (pad 18 thru_hole oval (at -2.54 20.32 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 29 "Net-(P2-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 20 thru_hole oval (at -2.54 22.86 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Multicomp_MC9A12-5034_2x25x2.54mm_Straight (layer B.Cu) (tedit 6139582A)
    (at 93.98 30.48 270)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference P9 (at -3.048 7.366 270) (layer B.SilkS))
    (fp_text value CON50 (at 30.48 -5 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 8 "Net-(P10-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 4 thru_hole circle (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 32 "Net-(P10-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 6 thru_hole circle (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 8 thru_hole circle (at 7.62 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 9 "Net-(P10-Pad8)"))
    (pad 9 thru_hole circle (at 10.16 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 10 thru_hole circle (at 10.16 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 12.7 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 12 thru_hole circle (at 12.7 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 15.24 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 14 thru_hole circle (at 15.24 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 10 "Net-(P10-Pad14)"))
    (pad 15 thru_hole circle (at 17.78 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 16 thru_hole circle (at 17.78 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 20.32 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 18 thru_hole circle (at 20.32 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 11 "Net-(P10-Pad18)"))
    (pad 19 thru_hole circle (at 22.86 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 20 thru_hole circle (at 22.86 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 12 "Net-(P10-Pad20)"))
    (pad 21 thru_hole circle (at 25.4 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 22 thru_hole circle (at 25.4 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 13 "Net-(P10-Pad22)"))
    (pad 23 thru_hole circle (at 27.94 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 24 thru_hole circle (at 27.94 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 30.48 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 26 thru_hole circle (at 30.48 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 14 "Net-(P10-Pad26)"))
    (pad 27 thru_hole circle (at 33.02 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 28 thru_hole circle (at 33.02 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 15 "Net-(P10-Pad28)"))
    (pad 29 thru_hole circle (at 35.56 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 30 thru_hole circle (at 35.56 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 16 "Net-(P10-Pad30)"))
    (pad 31 thru_hole circle (at 38.1 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 32 thru_hole circle (at 38.1 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 17 "Net-(P10-Pad32)"))
    (pad 33 thru_hole circle (at 40.64 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 34 thru_hole circle (at 40.64 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 18 "Net-(P10-Pad34)"))
    (pad 35 thru_hole circle (at 43.18 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 36 thru_hole circle (at 43.18 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 19 "Net-(P10-Pad24)"))
    (pad 37 thru_hole circle (at 45.72 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 38 thru_hole circle (at 45.72 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 48.26 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 40 thru_hole circle (at 48.26 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 20 "Net-(P10-Pad6)"))
    (pad 41 thru_hole circle (at 50.8 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 42 thru_hole circle (at 50.8 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 21 "Net-(P10-Pad10)"))
    (pad 43 thru_hole circle (at 53.34 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 44 thru_hole circle (at 53.34 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 22 "Net-(P10-Pad12)"))
    (pad 45 thru_hole circle (at 55.88 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 46 thru_hole circle (at 55.88 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at 58.42 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 48 thru_hole circle (at 58.42 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at 60.96 0 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 50 thru_hole circle (at 60.96 2.54 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask))
  )
  (module all_fp:Pin_Socket_Straight_2x17_Pitch2.54mm locked (layer F.Cu) (tedit 6139583B)
    (at 78.74 30.48)
    (descr "Through hole straight pin header, 2x17, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x17 2.54mm double row")
    (fp_text reference P11 (at -1.27 -3.048) (layer F.SilkS))
    (fp_text value CON34 (at -1.27 42.97) (layer F.Fab))
    (fp_text user %R (at -1.27 20.32 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 "Net-(P10-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 4 thru_hole oval (at -2.54 2.54 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 32 "Net-(P10-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 6 thru_hole oval (at -2.54 5.08 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 "Net-(P10-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 8 thru_hole oval (at -2.54 7.62 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(P10-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 10 thru_hole oval (at -2.54 10.16 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 "Net-(P10-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 12 thru_hole oval (at -2.54 12.7 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(P10-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 14 thru_hole oval (at -2.54 15.24 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(P10-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 16 thru_hole oval (at -2.54 17.78 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 18 thru_hole oval (at -2.54 20.32 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(P10-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 20 thru_hole oval (at -2.54 22.86 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(P10-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 22 thru_hole oval (at -2.54 25.4 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 13 "Net-(P10-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 24 thru_hole oval (at -2.54 27.94 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 19 "Net-(P10-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 26 thru_hole oval (at -2.54 30.48 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 "Net-(P10-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 28 thru_hole oval (at -2.54 33.02 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 "Net-(P10-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 30 thru_hole oval (at -2.54 35.56 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 "Net-(P10-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 32 thru_hole oval (at -2.54 38.1 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 "Net-(P10-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 34 thru_hole oval (at -2.54 40.64 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 "Net-(P10-Pad34)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x17_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:DIP-8_W7.62mm (layer F.Cu) (tedit 61395ADB)
    (at 105.41 129.54 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 10.16 90) (layer F.SilkS))
    (fp_text value 75LBC176 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "Net-(P2-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(P5-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "Net-(P2-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_2x10 (layer B.Cu) (tedit 5AA56437)
    (at 92.71 115.57 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at -5.08 -5.715 270) (layer B.SilkS))
    (fp_text value CON20_SA1000 (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at -11.43 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 3 thru_hole oval (at -8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS))
    (pad 4 thru_hole oval (at -8.89 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 5 thru_hole oval (at -6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS))
    (pad 6 thru_hole oval (at -6.35 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 7 thru_hole oval (at -3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole oval (at -3.81 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 9 thru_hole oval (at -1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 30 "Net-(P2-Pad9)"))
    (pad 10 thru_hole oval (at -1.27 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 31 "Net-(P2-Pad10)"))
    (pad 11 thru_hole oval (at 1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 12 thru_hole oval (at 1.27 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 13 thru_hole oval (at 3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 26 "Net-(P2-Pad13)"))
    (pad 14 thru_hole oval (at 3.81 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 27 "Net-(P2-Pad14)"))
    (pad 15 thru_hole oval (at 6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 16 thru_hole oval (at 6.35 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 17 thru_hole oval (at 8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 28 "Net-(P2-Pad17)"))
    (pad 18 thru_hole oval (at 8.89 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 29 "Net-(P2-Pad18)"))
    (pad 19 thru_hole oval (at 11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 20 thru_hole oval (at 11.43 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (model Pin_Headers/Pin_Header_Straight_2x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5AA5E3D0)
    (at 114.935 102.87 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 75 (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 23 GND))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(P1-Pad13)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5C662D0F)
    (at 100.965 113.03 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0 -2.667 90) (layer F.SilkS))
    (fp_text value 75 (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 23 GND))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(P1-Pad14)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer B.Cu) (tedit 613953DB)
    (at 85.725 121.92 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at -0.0508 -2.6924 90) (layer B.SilkS))
    (fp_text value 75 (at 3.81 -3.81 90) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 23 GND))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(P2-Pad17)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer B.Cu) (tedit 613953D0)
    (at 85.725 107.95 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at 0.2286 -2.667 90) (layer B.SilkS))
    (fp_text value 75 (at 3.81 -3.81 90) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 23 GND))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(P2-Pad18)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 6138058D)
    (at 100.076 147.32)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference F1 (at 1.524 -2.54) (layer F.SilkS))
    (fp_text value 2A (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 25 /24V))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 36 "Net-(C1-Pad2)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 61395AE0)
    (at 101.346 129.032 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C4 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value .1uf (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 +5V))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 6139572A)
    (at 91.948 141.224)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C5 (at -3.302 0.254 90) (layer F.SilkS))
    (fp_text value 18pF (at -1.016 3.048) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(C5-Pad2)"))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 61395733)
    (at 91.948 136.398)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C6 (at -3.302 0 90) (layer F.SilkS))
    (fp_text value 18pF (at -1.016 3.048) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(C6-Pad2)"))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:DIP-8_W7.62mm (layer F.Cu) (tedit 6139589D)
    (at 102.616 140.716 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at -2.286 3.048 180) (layer F.SilkS))
    (fp_text value ATTINY45-P (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad4)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:380999 (layer B.Cu) (tedit 613958D1)
    (at 88.9 149.86 90)
    (fp_text reference P3 (at 7.366 -12.7 90) (layer B.SilkS))
    (fp_text value CONN_01X06 (at -4.445 -2.286 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.794 2.794) (drill 1.778) (layers *.Cu *.Mask B.SilkS)
      (net 25 /24V))
    (pad 2 thru_hole circle (at -9.144 0 90) (size 2.794 2.794) (drill 1.778) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 3 thru_hole circle (at 0 -4.953 90) (size 2.794 2.794) (drill 1.778) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
    (pad 4 thru_hole circle (at -9.144 -4.953 90) (size 2.794 2.794) (drill 1.778) (layers *.Cu *.Mask B.SilkS))
    (pad 5 thru_hole circle (at 0 -9.906 90) (size 2.794 2.794) (drill 1.778) (layers *.Cu *.Mask B.SilkS)
      (net 24 +5V))
    (pad 6 thru_hole circle (at -9.144 -9.906 90) (size 2.794 2.794) (drill 1.778) (layers *.Cu *.Mask B.SilkS)
      (net 23 GND))
  )
  (module all_fp:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5AA5DB44)
    (at 116.84 135.89 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P5 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.778 1.778) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.778 1.778) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P5-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:esock20 locked (layer F.Cu) (tedit 6139586A)
    (at 110.49 93.345)
    (fp_text reference P6 (at -2.6416 -3.8608) (layer F.SilkS))
    (fp_text value CON20 (at -2.6416 17.3228 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -4.8514 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at -4.8514 2.54) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 5 thru_hole circle (at 0 5.08) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -4.8514 5.08) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 7 thru_hole circle (at 0 7.62) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -4.8514 7.62) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 9 thru_hole circle (at 0 10.16) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at -4.8514 10.16) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 11 thru_hole circle (at 0 12.7) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -4.8514 12.7) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 13 thru_hole circle (at 0 15.24) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad13)"))
    (pad 14 thru_hole circle (at -4.8514 15.24) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad14)"))
    (pad 15 thru_hole circle (at 0 17.78) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 16 thru_hole circle (at -4.8514 17.78) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 17 thru_hole circle (at 0 20.32) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad17)"))
    (pad 18 thru_hole circle (at -4.8514 20.32) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad18)"))
    (pad 19 thru_hole circle (at 0 22.86) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 20 thru_hole circle (at -4.8514 22.86) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
  )
  (module all_fp:esock34 locked (layer F.Cu) (tedit 6139584B)
    (at 110.49 30.48)
    (fp_text reference P10 (at -2.6416 -3.8608) (layer F.SilkS))
    (fp_text value CON34 (at -2.6416 17.3228 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 2 thru_hole circle (at -4.8514 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P10-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 4 thru_hole circle (at -4.8514 2.54) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P10-Pad4)"))
    (pad 5 thru_hole circle (at 0 5.08) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 6 thru_hole circle (at -4.8514 5.08) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P10-Pad6)"))
    (pad 7 thru_hole circle (at 0 7.62) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 8 thru_hole circle (at -4.8514 7.62) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P10-Pad8)"))
    (pad 9 thru_hole circle (at 0 10.16) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 10 thru_hole circle (at -4.8514 10.16) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P10-Pad10)"))
    (pad 11 thru_hole circle (at 0 12.7) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 12 thru_hole circle (at -4.8514 12.7) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P10-Pad12)"))
    (pad 13 thru_hole circle (at 0 15.24) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 14 thru_hole circle (at -4.8514 15.24) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P10-Pad14)"))
    (pad 15 thru_hole circle (at 0 17.78) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 16 thru_hole circle (at -4.8514 17.78) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 0 20.32) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 18 thru_hole circle (at -4.8514 20.32) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P10-Pad18)"))
    (pad 19 thru_hole circle (at 0 22.86) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 20 thru_hole circle (at -4.8514 22.86) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P10-Pad20)"))
    (pad 21 thru_hole circle (at 0 25.4) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 22 thru_hole circle (at -4.8514 25.4) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P10-Pad22)"))
    (pad 23 thru_hole circle (at 0 27.94) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 24 thru_hole circle (at -4.8514 27.94) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P10-Pad24)"))
    (pad 25 thru_hole circle (at 0 30.48) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 26 thru_hole circle (at -4.8514 30.48) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P10-Pad26)"))
    (pad 27 thru_hole circle (at 0 33.02) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 28 thru_hole circle (at -4.8514 33.02) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P10-Pad28)"))
    (pad 29 thru_hole circle (at 0 35.56) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 30 thru_hole circle (at -4.8514 35.56) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P10-Pad30)"))
    (pad 31 thru_hole circle (at 0 38.1) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 32 thru_hole circle (at -4.8514 38.1) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P10-Pad32)"))
    (pad 33 thru_hole circle (at 0 40.64) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 34 thru_hole circle (at -4.8514 40.64) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P10-Pad34)"))
  )
  (module all_fp:78SR-12 (layer F.Cu) (tedit 613958DF)
    (at 107.95 157.48)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference U2 (at 3.048 2.413 90) (layer F.SilkS))
    (fp_text value 78SR-12 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.0668) (layers *.Cu *.Mask)
      (net 36 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.778 1.778) (drill 1.0668) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.778 1.778) (drill 1.0668) (layers *.Cu *.Mask)
      (net 1 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Crystal_HC49-4H_Vertical (layer F.Cu) (tedit 613D166C)
    (at 97.536 141.224 90)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 8.128 -3.81 90) (layer F.SilkS))
    (fp_text value "18.432 MHz" (at 2.44 3.525 90) (layer F.Fab))
    (fp_text user %R (at 2.44 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 4.88 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "SA1000 Rev D\nwww.pdp8online.com/mfm" (at 76.962 124.968 90) (layer F.SilkS))
  (gr_text 1 (at 98.425 104.14 90) (layer B.SilkS))
  (gr_text 1 (at 98.425 29.845 90) (layer B.SilkS))
  (gr_text 1 (at 81.915 82.55 90) (layer F.SilkS))
  (gr_text 1 (at 81.915 30.48 90) (layer F.SilkS))
  (gr_text 1 (at 113.665 30.48 90) (layer F.SilkS))
  (gr_text 1 (at 113.665 93.345 90) (layer F.SilkS))
  (gr_line (start 130.81 33.909) (end 130.81 28.956) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 33.909) (end 130.81 33.909) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 34.671) (end 119.38 33.909) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 34.671) (end 119.38 34.671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 92.837) (end 130.81 34.671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 139.954) (end 120.65 132.461) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 139.954) (end 120.65 139.954) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 167.894) (end 130.81 139.954) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.39 167.894) (end 130.81 167.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.39 165.354) (end 72.39 167.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.39 23.114) (end 72.39 165.354) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 23.114) (end 72.39 23.114) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 28.194) (end 120.65 23.114) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.286 28.194) (end 120.65 28.194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 28.956) (end 129.286 28.194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.286 93.599) (end 130.81 92.837) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 93.599) (end 129.286 93.599) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 105.029) (end 120.65 93.599) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.286 105.029) (end 120.65 105.029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 105.791) (end 129.286 105.029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 110.744) (end 130.81 105.791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 110.744) (end 130.81 110.744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 111.506) (end 119.38 110.744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 111.506) (end 119.38 111.506) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 131.699) (end 130.81 111.506) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.286 132.461) (end 130.81 131.699) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.65 132.461) (end 129.286 132.461) (layer Edge.Cuts) (width 0.1))
  (gr_text "CLK EN" (at 114.3 135.89 90) (layer F.SilkS))
  (zone (net 23) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.54 167.132) (xy 73.152 167.132) (xy 73.152 23.876) (xy 119.38 23.876) (xy 119.38 141.224)
        (xy 129.54 141.224)
      )
    )
  )
  (zone (net 23) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.54 167.132) (xy 73.152 167.132) (xy 73.152 23.876) (xy 119.38 23.876) (xy 119.38 141.224)
        (xy 129.54 141.224)
      )
    )
  )
)
