(kicad_pcb (version 3) (host pcbnew "(2014-02-12 BZR 4693)-product")
  (general
    (links 359)
    (no_connects 0)
    (area 107.378499 10.38352 234.645201 165.58768)
    (thickness 1.6)
    (drawings 54)
    (tracks 1590)
    (zones 0)
    (modules 81)
    (nets 174)
  )
  (page USLetter)
  (title_block
    (title "MFM Disk Reader and Emulator")
    (date "18 May 2014")
    (rev 1)
    (company "David Gesswein")
  )
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user hide)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2032)
    (edge_width 0.1016)
    (via_size 0.889)
    (via_drill 0.508)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.254)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.254)
    (pad_size 1.778 1.778)
    (pad_drill 0.8128)
    (pad_to_mask_clearance 0.06)
    (aux_axis_origin 0 0)
    (grid_origin 97.155 15.24)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 284196865)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 +5V)
  (net 3 /emu/DIR_IN)
  (net 4 /emu/EXPANSION0)
  (net 5 /emu/EXPANSION1)
  (net 6 /emu/EXPANSION10)
  (net 7 /emu/EXPANSION11)
  (net 8 /emu/EXPANSION12)
  (net 9 /emu/EXPANSION13)
  (net 10 /emu/EXPANSION2)
  (net 11 /emu/EXPANSION3)
  (net 12 /emu/EXPANSION4)
  (net 13 /emu/EXPANSION5)
  (net 14 /emu/EXPANSION6)
  (net 15 /emu/EXPANSION7)
  (net 16 /emu/EXPANSION8)
  (net 17 /emu/EXPANSION9)
  (net 18 /emu/E_DIR_IN)
  (net 19 /emu/E_HEAD0)
  (net 20 /emu/E_HEAD1)
  (net 21 /emu/E_HEAD2)
  (net 22 /emu/E_HEAD3)
  (net 23 /emu/E_SEL1)
  (net 24 /emu/E_SEL2)
  (net 25 /emu/E_SEL3)
  (net 26 /emu/E_SEL4)
  (net 27 /emu/E_STEP)
  (net 28 /emu/E_UNUSED)
  (net 29 /emu/E_WRITE)
  (net 30 /emu/HEAD0)
  (net 31 /emu/HEAD1)
  (net 32 /emu/HEAD2)
  (net 33 /emu/HEAD3)
  (net 34 /emu/INDEX)
  (net 35 /emu/READY)
  (net 36 /emu/RECOVERY)
  (net 37 /emu/SEEK_DONE)
  (net 38 /emu/SEL1)
  (net 39 /emu/SEL2)
  (net 40 /emu/SEL3)
  (net 41 /emu/SEL4)
  (net 42 /emu/SELECTED)
  (net 43 /emu/STEP)
  (net 44 /emu/TRACK0)
  (net 45 /emu/WFAULT)
  (net 46 /emu/WRITE)
  (net 47 /emu/~EMU_EN)
  (net 48 /emu/~MFM0_IN)
  (net 49 /emu/~MFM_READ_EN)
  (net 50 AGND)
  (net 51 GND)
  (net 52 I2C2_SCL)
  (net 53 I2C2_SDA)
  (net 54 MFM_DATA)
  (net 55 "Net-(C1-Pad1)")
  (net 56 "Net-(C1-Pad2)")
  (net 57 "Net-(C2-Pad2)")
  (net 58 "Net-(C3-Pad2)")
  (net 59 "Net-(C4-Pad2)")
  (net 60 "Net-(C6-Pad1)")
  (net 61 "Net-(D1-Pad1)")
  (net 62 "Net-(D1-Pad2)")
  (net 63 "Net-(D2-Pad1)")
  (net 64 "Net-(J1-Pad1)")
  (net 65 "Net-(J1-Pad10)")
  (net 66 "Net-(J1-Pad13)")
  (net 67 "Net-(J1-Pad14)")
  (net 68 "Net-(J1-Pad17)")
  (net 69 "Net-(J1-Pad18)")
  (net 70 "Net-(J1-Pad3)")
  (net 71 "Net-(J1-Pad5)")
  (net 72 "Net-(J1-Pad7)")
  (net 73 "Net-(J1-Pad9)")
  (net 74 "Net-(J2-Pad10)")
  (net 75 "Net-(J2-Pad12)")
  (net 76 "Net-(J2-Pad16)")
  (net 77 "Net-(J2-Pad20)")
  (net 78 "Net-(J2-Pad22)")
  (net 79 "Net-(J2-Pad8)")
  (net 80 "Net-(J3-Pad1)")
  (net 81 "Net-(J3-Pad10)")
  (net 82 "Net-(J3-Pad3)")
  (net 83 "Net-(J3-Pad5)")
  (net 84 "Net-(J3-Pad7)")
  (net 85 "Net-(J3-Pad9)")
  (net 86 "Net-(J4-Pad10)")
  (net 87 "Net-(J4-Pad12)")
  (net 88 "Net-(J4-Pad14)")
  (net 89 "Net-(J4-Pad18)")
  (net 90 "Net-(J4-Pad2)")
  (net 91 "Net-(J4-Pad20)")
  (net 92 "Net-(J4-Pad22)")
  (net 93 "Net-(J4-Pad24)")
  (net 94 "Net-(J4-Pad26)")
  (net 95 "Net-(J4-Pad28)")
  (net 96 "Net-(J4-Pad30)")
  (net 97 "Net-(J4-Pad32)")
  (net 98 "Net-(J4-Pad34)")
  (net 99 "Net-(J4-Pad4)")
  (net 100 "Net-(J4-Pad6)")
  (net 101 "Net-(J4-Pad8)")
  (net 102 "Net-(J5-Pad4)")
  (net 103 "Net-(J6-Pad10)")
  (net 104 "Net-(J6-Pad13)")
  (net 105 "Net-(J6-Pad14)")
  (net 106 "Net-(J6-Pad17)")
  (net 107 "Net-(J6-Pad18)")
  (net 108 "Net-(J6-Pad3)")
  (net 109 "Net-(J6-Pad5)")
  (net 110 "Net-(J6-Pad7)")
  (net 111 "Net-(J6-Pad9)")
  (net 112 "Net-(P1-Pad1)")
  (net 113 "Net-(P4-Pad2)")
  (net 114 "Net-(P4-Pad4)")
  (net 115 "Net-(R19-Pad1)")
  (net 116 "Net-(R3-Pad2)")
  (net 117 "Net-(R6-Pad1)")
  (net 118 "Net-(U1-PadB16)")
  (net 119 "Net-(U1-PadB20)")
  (net 120 "Net-(U1-PadB21)")
  (net 121 "Net-(U1-PadB22)")
  (net 122 "Net-(U1-PadB23)")
  (net 123 "Net-(U1-PadB24)")
  (net 124 "Net-(U1-PadB25)")
  (net 125 "Net-(U1-PadB26)")
  (net 126 "Net-(U1-PadB3)")
  (net 127 "Net-(U1-PadB31)")
  (net 128 "Net-(U1-PadB32)")
  (net 129 "Net-(U1-PadB33)")
  (net 130 "Net-(U1-PadB34)")
  (net 131 "Net-(U1-PadB35)")
  (net 132 "Net-(U1-PadB36)")
  (net 133 "Net-(U1-PadB37)")
  (net 134 "Net-(U1-PadB38)")
  (net 135 "Net-(U1-PadB39)")
  (net 136 "Net-(U1-PadB4)")
  (net 137 "Net-(U1-PadB40)")
  (net 138 "Net-(U1-PadB41)")
  (net 139 "Net-(U1-PadB42)")
  (net 140 "Net-(U1-PadB44)")
  (net 141 "Net-(U1-PadB5)")
  (net 142 "Net-(U1-PadB6)")
  (net 143 "Net-(U1-PadC10)")
  (net 144 "Net-(U1-PadC15)")
  (net 145 "Net-(U1-PadC16)")
  (net 146 "Net-(U1-PadC23)")
  (net 147 "Net-(U1-PadC32)")
  (net 148 "Net-(U1-PadC33)")
  (net 149 "Net-(U1-PadC35)")
  (net 150 "Net-(U1-PadC36)")
  (net 151 "Net-(U1-PadC37)")
  (net 152 "Net-(U1-PadC38)")
  (net 153 "Net-(U1-PadC40)")
  (net 154 "Net-(U1-PadC7)")
  (net 155 "Net-(U1-PadC8)")
  (net 156 "Net-(U1-PadC9)")
  (net 157 "Net-(U11-Pad7)")
  (net 158 "Net-(U12-Pad1)")
  (net 159 "Net-(U12-Pad6)")
  (net 160 "Net-(U13-Pad1)")
  (net 161 "Net-(U13-Pad8)")
  (net 162 "Net-(U2-Pad6)")
  (net 163 "Net-(U3-Pad6)")
  (net 164 "Net-(U3-Pad7)")
  (net 165 "Net-(U3-Pad8)")
  (net 166 "Net-(U3-Pad9)")
  (net 167 "Net-(U4-Pad1)")
  (net 168 "Net-(U4-Pad8)")
  (net 169 "Net-(U5-Pad8)")
  (net 170 "Net-(U5-Pad9)")
  (net 171 RECOVERY_DRIVE2_SEL)
  (net 172 V12_ADC)
  (net 173 ~MFM1_IN)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +3.3V)
    (add_net +5V)
    (add_net /emu/DIR_IN)
    (add_net /emu/EXPANSION0)
    (add_net /emu/EXPANSION1)
    (add_net /emu/EXPANSION10)
    (add_net /emu/EXPANSION11)
    (add_net /emu/EXPANSION12)
    (add_net /emu/EXPANSION13)
    (add_net /emu/EXPANSION2)
    (add_net /emu/EXPANSION3)
    (add_net /emu/EXPANSION4)
    (add_net /emu/EXPANSION5)
    (add_net /emu/EXPANSION6)
    (add_net /emu/EXPANSION7)
    (add_net /emu/EXPANSION8)
    (add_net /emu/EXPANSION9)
    (add_net /emu/E_DIR_IN)
    (add_net /emu/E_HEAD0)
    (add_net /emu/E_HEAD1)
    (add_net /emu/E_HEAD2)
    (add_net /emu/E_HEAD3)
    (add_net /emu/E_SEL1)
    (add_net /emu/E_SEL2)
    (add_net /emu/E_SEL3)
    (add_net /emu/E_SEL4)
    (add_net /emu/E_STEP)
    (add_net /emu/E_UNUSED)
    (add_net /emu/E_WRITE)
    (add_net /emu/HEAD0)
    (add_net /emu/HEAD1)
    (add_net /emu/HEAD2)
    (add_net /emu/HEAD3)
    (add_net /emu/INDEX)
    (add_net /emu/READY)
    (add_net /emu/RECOVERY)
    (add_net /emu/SEEK_DONE)
    (add_net /emu/SEL1)
    (add_net /emu/SEL2)
    (add_net /emu/SEL3)
    (add_net /emu/SEL4)
    (add_net /emu/SELECTED)
    (add_net /emu/STEP)
    (add_net /emu/TRACK0)
    (add_net /emu/WFAULT)
    (add_net /emu/WRITE)
    (add_net /emu/~EMU_EN)
    (add_net /emu/~MFM0_IN)
    (add_net /emu/~MFM_READ_EN)
    (add_net AGND)
    (add_net GND)
    (add_net I2C2_SCL)
    (add_net I2C2_SDA)
    (add_net MFM_DATA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J4-Pad18)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad20)")
    (add_net "Net-(J4-Pad22)")
    (add_net "Net-(J4-Pad24)")
    (add_net "Net-(J4-Pad26)")
    (add_net "Net-(J4-Pad28)")
    (add_net "Net-(J4-Pad30)")
    (add_net "Net-(J4-Pad32)")
    (add_net "Net-(J4-Pad34)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J6-Pad10)")
    (add_net "Net-(J6-Pad13)")
    (add_net "Net-(J6-Pad14)")
    (add_net "Net-(J6-Pad17)")
    (add_net "Net-(J6-Pad18)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J6-Pad7)")
    (add_net "Net-(J6-Pad9)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(U1-PadB16)")
    (add_net "Net-(U1-PadB20)")
    (add_net "Net-(U1-PadB21)")
    (add_net "Net-(U1-PadB22)")
    (add_net "Net-(U1-PadB23)")
    (add_net "Net-(U1-PadB24)")
    (add_net "Net-(U1-PadB25)")
    (add_net "Net-(U1-PadB26)")
    (add_net "Net-(U1-PadB3)")
    (add_net "Net-(U1-PadB31)")
    (add_net "Net-(U1-PadB32)")
    (add_net "Net-(U1-PadB33)")
    (add_net "Net-(U1-PadB34)")
    (add_net "Net-(U1-PadB35)")
    (add_net "Net-(U1-PadB36)")
    (add_net "Net-(U1-PadB37)")
    (add_net "Net-(U1-PadB38)")
    (add_net "Net-(U1-PadB39)")
    (add_net "Net-(U1-PadB4)")
    (add_net "Net-(U1-PadB40)")
    (add_net "Net-(U1-PadB41)")
    (add_net "Net-(U1-PadB42)")
    (add_net "Net-(U1-PadB44)")
    (add_net "Net-(U1-PadB5)")
    (add_net "Net-(U1-PadB6)")
    (add_net "Net-(U1-PadC10)")
    (add_net "Net-(U1-PadC15)")
    (add_net "Net-(U1-PadC16)")
    (add_net "Net-(U1-PadC23)")
    (add_net "Net-(U1-PadC32)")
    (add_net "Net-(U1-PadC33)")
    (add_net "Net-(U1-PadC35)")
    (add_net "Net-(U1-PadC36)")
    (add_net "Net-(U1-PadC37)")
    (add_net "Net-(U1-PadC38)")
    (add_net "Net-(U1-PadC40)")
    (add_net "Net-(U1-PadC7)")
    (add_net "Net-(U1-PadC8)")
    (add_net "Net-(U1-PadC9)")
    (add_net "Net-(U11-Pad7)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U12-Pad6)")
    (add_net "Net-(U13-Pad1)")
    (add_net "Net-(U13-Pad8)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U5-Pad9)")
    (add_net RECOVERY_DRIVE2_SEL)
    (add_net V12_ADC)
    (add_net ~MFM1_IN)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 1.27)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module all_fp:ECON34 (layer F.Cu) (tedit 53A39C81)
    (at 222.885 82.8802 90)
    (fp_text reference J2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value ECON34 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user 33 (at -21.5138 -0.381 90) (layer F.SilkS))
    (fp_text user 1 (at 18.8468 -0.7112 90) (layer F.SilkS))
    (pad 1 connect rect (at 18.9992 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 2 connect rect (at 18.9992 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 22 /emu/E_HEAD3))
    (pad 3 connect rect (at 16.4592 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 4 connect rect (at 16.4592 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 21 /emu/E_HEAD2))
    (pad 5 connect rect (at 13.9192 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 6 connect rect (at 13.9192 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 29 /emu/E_WRITE))
    (pad 7 connect rect (at 11.3792 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 8 connect rect (at 11.3792 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 79 "Net-(J2-Pad8)"))
    (pad 9 connect rect (at 8.8392 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 10 connect rect (at 8.8392 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 74 "Net-(J2-Pad10)"))
    (pad 11 connect rect (at 6.2992 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 12 connect rect (at 6.2992 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 75 "Net-(J2-Pad12)"))
    (pad 13 connect rect (at 3.7592 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 14 connect rect (at 3.7592 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 19 /emu/E_HEAD0))
    (pad 15 connect rect (at 1.2192 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 16 connect rect (at 1.2192 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 76 "Net-(J2-Pad16)"))
    (pad 17 connect rect (at -1.3208 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 18 connect rect (at -1.3208 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 20 /emu/E_HEAD1))
    (pad 19 connect rect (at -3.8608 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 20 connect rect (at -3.8608 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 77 "Net-(J2-Pad20)"))
    (pad 21 connect rect (at -6.4008 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 22 connect rect (at -6.4008 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 78 "Net-(J2-Pad22)"))
    (pad 23 connect rect (at -8.9408 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 24 connect rect (at -8.9408 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 27 /emu/E_STEP))
    (pad 25 connect rect (at -11.4808 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 26 connect rect (at -11.4808 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 23 /emu/E_SEL1))
    (pad 27 connect rect (at -14.0208 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 28 connect rect (at -14.0208 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 24 /emu/E_SEL2))
    (pad 29 connect rect (at -16.5608 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 30 connect rect (at -16.5608 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 25 /emu/E_SEL3))
    (pad 31 connect rect (at -19.1008 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 32 connect rect (at -19.1008 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 26 /emu/E_SEL4))
    (pad 33 connect rect (at -21.6408 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 34 connect rect (at -21.6408 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 18 /emu/E_DIR_IN))
  )
  (module all_fp:econ20 (layer F.Cu) (tedit 53A39B15)
    (at 228.981 136.804 90)
    (fp_text reference J1 (at -0.381 -6.35 90) (layer F.SilkS))
    (fp_text value ECON20 (at -5.08 0 90) (layer F.SilkS) hide)
    (fp_text user 19 (at -12.7 -6.477 90) (layer F.SilkS))
    (fp_text user 1 (at 9.906 -6.477 90) (layer F.SilkS))
    (pad 1 connect rect (at 10.0584 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 64 "Net-(J1-Pad1)"))
    (pad 2 connect rect (at 10.0584 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 51 GND))
    (pad 3 connect rect (at 7.5184 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 70 "Net-(J1-Pad3)"))
    (pad 4 connect rect (at 7.5184 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 51 GND))
    (pad 5 connect rect (at 4.9784 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 71 "Net-(J1-Pad5)"))
    (pad 6 connect rect (at 4.9784 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 51 GND))
    (pad 7 connect rect (at 2.4384 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 72 "Net-(J1-Pad7)"))
    (pad 8 connect rect (at 2.4384 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 51 GND))
    (pad 9 connect rect (at -0.1016 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 73 "Net-(J1-Pad9)"))
    (pad 10 connect rect (at -0.1016 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 65 "Net-(J1-Pad10)"))
    (pad 11 connect rect (at -2.6416 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 12 connect rect (at -2.6416 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 51 GND))
    (pad 13 connect rect (at -5.1816 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 66 "Net-(J1-Pad13)"))
    (pad 14 connect rect (at -5.1816 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 67 "Net-(J1-Pad14)"))
    (pad 15 connect rect (at -7.7216 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 16 connect rect (at -7.7216 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 51 GND))
    (pad 17 connect rect (at -10.2616 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 68 "Net-(J1-Pad17)"))
    (pad 18 connect rect (at -10.2616 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 69 "Net-(J1-Pad18)"))
    (pad 19 connect rect (at -12.8016 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 51 GND))
    (pad 20 connect rect (at -12.8016 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 51 GND))
  )
  (module all_fp:DRVPWR (layer F.Cu) (tedit 5399035F)
    (at 215.138 34.544 270)
    (fp_text reference J5 (at -1.905 -1.3335 270) (layer F.SilkS))
    (fp_text value CONN_4 (at -1.27 -10.16 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 6.35 -5.08 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -5.08 270) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 3 thru_hole circle (at -3.81 -5.08 270) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 4 thru_hole circle (at -8.89 -5.08 270) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(J5-Pad4)"))
    (pad "" np_thru_hole circle (at -6.35 -15.24 270) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 3.81 -15.24 270) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -11.43 -7.62 270) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 8.89 -7.62 270) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (model /home/djg/mfm/all_fp.pretty/DRVPWR.wrl
      (at (xyz -0.05 0.21 0.185))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz -90 0 180))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 539906A0)
    (at 150.114 49.657 90)
    (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 5mm 5MM 100mil 2,54mm")
    (fp_text reference D2 (at 4.191 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/leds/led5_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM20mm (layer F.Cu) (tedit 53A44BCC)
    (at 189.865 53.721 180)
    (descr "Resistor, Axial, RM 20mm,")
    (tags "Resistor, Axial, RM 20mm,")
    (fp_text reference R13 (at -1.4605 -4.1275 180) (layer F.SilkS))
    (fp_text value 8.2 (at 0 5.00126 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -9.99998 0 180) (size 1.99898 1.99898) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 62 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 10.32002 0 180) (size 1.99898 1.99898) (drill 1.0922) (layers *.Cu *.SilkS *.Mask)
      (net 55 "Net-(C1-Pad1)"))
    (model discret/resistors/horizontal/r_h_8R2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-201AD_Horizontal_RM15 (layer F.Cu) (tedit 53A44BDD)
    (at 207.772 36.449 270)
    (descr "Diode DO-201AD Horizontal")
    (tags "Diode DO-201AD Horizontal SB320 SB340 SB360")
    (fp_text reference D1 (at 0.5715 -4.318 270) (layer F.SilkS))
    (fp_text value 1N5820 (at 0.508 -4.826 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -7.62 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(D1-Pad1)"))
    (pad 2 thru_hole rect (at 7.62 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(D1-Pad2)"))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-201AD_Horizontal_RM15 (layer F.Cu) (tedit 537805D4)
    (at 167.005 47.244)
    (descr "Diode DO-201AD Horizontal")
    (tags "Diode DO-201AD Horizontal SB320 SB340 SB360")
    (fp_text reference D3 (at 0 -4.064) (layer F.SilkS))
    (fp_text value 1N5820 (at 0.508 -0.762) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -7.62 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C1-Pad1)"))
    (pad 2 thru_hole rect (at 7.62 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(D1-Pad2)"))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 5389147B)
    (at 195.453 80.264 270)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U14 (at -10.033 5.461 360) (layer F.SilkS))
    (fp_text value 7407N (at 1.27 1.27 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /emu/SEEK_DONE))
    (pad 2 thru_hole circle (at -5.08 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(J2-Pad8)"))
    (pad 3 thru_hole circle (at -2.54 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /emu/WFAULT))
    (pad 4 thru_hole circle (at 0 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J2-Pad12)"))
    (pad 5 thru_hole circle (at 2.54 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /emu/SELECTED))
    (pad 6 thru_hole circle (at 5.08 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(J1-Pad1)"))
    (pad 7 thru_hole circle (at 7.62 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J2-Pad22)"))
    (pad 9 thru_hole circle (at 5.08 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /emu/READY))
    (pad 10 thru_hole circle (at 2.54 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J2-Pad20)"))
    (pad 11 thru_hole circle (at 0 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /emu/INDEX))
    (pad 12 thru_hole circle (at -2.54 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J2-Pad10)"))
    (pad 13 thru_hole circle (at -5.08 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /emu/TRACK0))
    (pad 14 thru_hole circle (at -7.62 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 53990219)
    (at 141.859 122.047)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U15 (at -9.906 -5.334 90) (layer F.SilkS))
    (fp_text value 7407N (at 1.27 1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /emu/WRITE))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(P1-Pad1)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /emu/HEAD2))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(J4-Pad4)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /emu/HEAD0))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J4-Pad14)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J4-Pad18)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /emu/HEAD1))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 171 RECOVERY_DRIVE2_SEL))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /emu/RECOVERY))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(J4-Pad2)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /emu/HEAD3))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 53990A51)
    (at 168.021 121.92)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U16 (at -10.16 5.461 90) (layer F.SilkS))
    (fp_text value 7407N (at 3.048 -0.254) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /emu/STEP))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(J4-Pad24)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /emu/SEL2))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(J4-Pad28)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /emu/SEL4))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(J4-Pad32)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(J4-Pad34)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /emu/DIR_IN))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(J4-Pad30)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /emu/SEL3))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(J4-Pad26)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /emu/SEL1))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5399020C)
    (at 123.825 122.682 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at -4.064 0.0635 270) (layer F.SilkS))
    (fp_text value CONN_1X2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(J4-Pad6)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 5397BFEE)
    (at 176.657 83.566)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P4 (at 4.826 0.254) (layer F.SilkS))
    (fp_text value CONN_2X2 (at -0.549409 4.1672) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole oval (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 4 thru_hole oval (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(P4-Pad4)"))
    (model Pin_Headers/Pin_Header_Straight_2x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-20__300 (layer F.Cu) (tedit 536EE181)
    (at 208.407 71.882 270)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U2 (at -13.97 4.445 360) (layer F.SilkS))
    (fp_text value 74LVC245 (at 6.35 1.27 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole circle (at -8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /emu/HEAD3))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /emu/HEAD2))
    (pad 4 thru_hole circle (at -3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /emu/WRITE))
    (pad 5 thru_hole circle (at -1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /emu/HEAD0))
    (pad 6 thru_hole circle (at 1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /emu/HEAD1))
    (pad 8 thru_hole circle (at 6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /emu/STEP))
    (pad 9 thru_hole circle (at 8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /emu/SEL1))
    (pad 10 thru_hole circle (at 11.43 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /emu/E_SEL1))
    (pad 12 thru_hole circle (at 8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /emu/E_STEP))
    (pad 13 thru_hole circle (at 6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /emu/E_HEAD1))
    (pad 14 thru_hole circle (at 3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /emu/E_UNUSED))
    (pad 15 thru_hole circle (at 1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /emu/E_HEAD0))
    (pad 16 thru_hole circle (at -1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /emu/E_WRITE))
    (pad 17 thru_hole circle (at -3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /emu/E_HEAD2))
    (pad 18 thru_hole circle (at -6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /emu/E_HEAD3))
    (pad 19 thru_hole circle (at -8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /emu/~EMU_EN))
    (pad 20 thru_hole circle (at -11.43 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-20__300 (layer F.Cu) (tedit 5378057C)
    (at 208.28 105.791 270)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U3 (at -13.589 4.953 360) (layer F.SilkS))
    (fp_text value 74LVC245 (at 6.35 1.27 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole circle (at -8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /emu/SEL2))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /emu/SEL3))
    (pad 4 thru_hole circle (at -3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /emu/SEL4))
    (pad 5 thru_hole circle (at -1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /emu/DIR_IN))
    (pad 6 thru_hole circle (at 1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(U3-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 164 "Net-(U3-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 165 "Net-(U3-Pad8)"))
    (pad 9 thru_hole circle (at 8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 166 "Net-(U3-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(R3-Pad2)"))
    (pad 12 thru_hole circle (at 8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(R3-Pad2)"))
    (pad 13 thru_hole circle (at 6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(R3-Pad2)"))
    (pad 14 thru_hole circle (at 3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(R3-Pad2)"))
    (pad 15 thru_hole circle (at 1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /emu/E_DIR_IN))
    (pad 16 thru_hole circle (at -1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /emu/E_SEL4))
    (pad 17 thru_hole circle (at -3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /emu/E_SEL3))
    (pad 18 thru_hole circle (at -6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /emu/E_SEL2))
    (pad 19 thru_hole circle (at -8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /emu/~EMU_EN))
    (pad 20 thru_hole circle (at -11.43 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 5378055A)
    (at 178.638 136.652)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U4 (at -10.414 -4.572 270) (layer F.SilkS))
    (fp_text value MAX3491 (at 1.27 1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 167 "Net-(U4-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 MFM_DATA))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /emu/~MFM0_IN))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 MFM_DATA))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 168 "Net-(U4-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J1-Pad17)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J1-Pad18)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J1-Pad14)"))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J1-Pad13)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-20__300 (layer F.Cu) (tedit 5389143C)
    (at 141.224 134.112)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U5 (at -13.97 -4.572 90) (layer F.SilkS))
    (fp_text value 74LVC245 (at 6.35 1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(J4-Pad8)"))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J4-Pad10)"))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J4-Pad12)"))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(J4-Pad20)"))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(J4-Pad22)"))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J3-Pad1)"))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 169 "Net-(U5-Pad8)"))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 170 "Net-(U5-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(R6-Pad1)"))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(R6-Pad1)"))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /emu/SELECTED))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /emu/READY))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /emu/INDEX))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /emu/WFAULT))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /emu/TRACK0))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /emu/SEEK_DONE))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /emu/~MFM_READ_EN))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-8__300 (layer F.Cu) (tedit 5389DE0C)
    (at 172.339 74.422)
    (descr "8 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U11 (at 6.416 -0.4175 90) (layer F.SilkS))
    (fp_text value 24C256W (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(P4-Pad2)"))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(P4-Pad4)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 I2C2_SDA))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 I2C2_SCL))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(U11-Pad7)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 53990243)
    (at 194.945 127.254 270)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U13 (at -10.16 -5.461 360) (layer F.SilkS))
    (fp_text value MAX3491 (at 1.27 1.27 450) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 160 "Net-(U13-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 MFM_DATA))
    (pad 3 thru_hole circle (at -2.54 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 173 ~MFM1_IN))
    (pad 4 thru_hole circle (at 0 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 5 thru_hole circle (at 2.54 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 MFM_DATA))
    (pad 6 thru_hole circle (at 5.08 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 7 thru_hole circle (at 7.62 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(U13-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(J6-Pad17)"))
    (pad 10 thru_hole circle (at 2.54 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(J6-Pad18)"))
    (pad 11 thru_hole circle (at 0 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(J6-Pad14)"))
    (pad 12 thru_hole circle (at -2.54 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(J6-Pad13)"))
    (pad 13 thru_hole circle (at -5.08 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 14 thru_hole circle (at -7.62 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 536EDDD8)
    (at 147.955 86.36 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J7 (at -0.635 5.715 270) (layer F.SilkS))
    (fp_text value CONN_20 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole oval (at -11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 3 thru_hole oval (at -8.89 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /emu/EXPANSION5))
    (pad 4 thru_hole oval (at -8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /emu/EXPANSION0))
    (pad 5 thru_hole oval (at -6.35 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /emu/EXPANSION9))
    (pad 6 thru_hole oval (at -6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /emu/EXPANSION1))
    (pad 7 thru_hole oval (at -3.81 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /emu/EXPANSION8))
    (pad 8 thru_hole oval (at -3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /emu/EXPANSION3))
    (pad 9 thru_hole oval (at -1.27 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /emu/EXPANSION6))
    (pad 10 thru_hole oval (at -1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /emu/EXPANSION12))
    (pad 11 thru_hole oval (at 1.27 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /emu/EXPANSION7))
    (pad 12 thru_hole oval (at 1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /emu/EXPANSION11))
    (pad 13 thru_hole oval (at 3.81 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /emu/EXPANSION2))
    (pad 14 thru_hole oval (at 3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /emu/EXPANSION10))
    (pad 15 thru_hole oval (at 6.35 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /emu/EXPANSION13))
    (pad 16 thru_hole oval (at 6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /emu/EXPANSION4))
    (pad 17 thru_hole oval (at 8.89 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 I2C2_SCL))
    (pad 18 thru_hole oval (at 8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 I2C2_SDA))
    (pad 19 thru_hole oval (at 11.43 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 20 thru_hole oval (at 11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model Pin_Headers/Pin_Header_Straight_2x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 536F744D)
    (at 215.265 138.176 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at 0 -5.715 90) (layer F.SilkS))
    (fp_text value ECON20 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 171 RECOVERY_DRIVE2_SEL))
    (pad 2 thru_hole oval (at -11.43 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 3 thru_hole oval (at -8.89 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(J6-Pad3)"))
    (pad 4 thru_hole oval (at -8.89 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 5 thru_hole oval (at -6.35 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at -6.35 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 7 thru_hole oval (at -3.81 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(J6-Pad7)"))
    (pad 8 thru_hole oval (at -3.81 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 9 thru_hole oval (at -1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(J6-Pad9)"))
    (pad 10 thru_hole oval (at -1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(J6-Pad10)"))
    (pad 11 thru_hole oval (at 1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 12 thru_hole oval (at 1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 13 thru_hole oval (at 3.81 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(J6-Pad13)"))
    (pad 14 thru_hole oval (at 3.81 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(J6-Pad14)"))
    (pad 15 thru_hole oval (at 6.35 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 16 thru_hole oval (at 6.35 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 17 thru_hole oval (at 8.89 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(J6-Pad17)"))
    (pad 18 thru_hole oval (at 8.89 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(J6-Pad18)"))
    (pad 19 thru_hole oval (at 11.43 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 20 thru_hole oval (at 11.43 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model Pin_Headers/Pin_Header_Straight_2x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 5389153A)
    (at 189.611 148.336)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at -1.27 -5.715) (layer F.SilkS))
    (fp_text value CON20 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at -11.43 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 3 thru_hole oval (at -8.89 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at -8.89 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 5 thru_hole oval (at -6.35 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at -6.35 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 7 thru_hole oval (at -3.81 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at -3.81 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 9 thru_hole oval (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J3-Pad9)"))
    (pad 10 thru_hole oval (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J3-Pad10)"))
    (pad 11 thru_hole oval (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 12 thru_hole oval (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 13 thru_hole oval (at 3.81 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J1-Pad17)"))
    (pad 14 thru_hole oval (at 3.81 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J1-Pad18)"))
    (pad 15 thru_hole oval (at 6.35 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 16 thru_hole oval (at 6.35 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 17 thru_hole oval (at 8.89 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J1-Pad13)"))
    (pad 18 thru_hole oval (at 8.89 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J1-Pad14)"))
    (pad 19 thru_hole oval (at 11.43 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 20 thru_hole oval (at 11.43 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model Pin_Headers/Pin_Header_Straight_2x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:screw-6-32 (layer F.Cu) (tedit 53A45435)
    (at 111.887 158.115)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH3 (at 5.969 -1.397) (layer F.SilkS) hide)
    (fp_text value 6-32 (at 0 5.99948) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 -0.254) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
  )
  (module all_fp:screw-6-32 (layer B.Cu) (tedit 53A3970C)
    (at 191.135 157.861)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH2 (at 5.969 1.397) (layer B.SilkS) hide)
    (fp_text value 6-32 (at 0 -5.99948) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 0) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask B.SilkS))
  )
  (module all_fp:screw-6-32 (layer B.Cu) (tedit 5389D9FA)
    (at 191.135 18.161)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH4 (at 5.969 1.397) (layer B.SilkS) hide)
    (fp_text value 6-32 (at 0 -5.99948) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 0) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask B.SilkS))
  )
  (module all_fp:screw-6-32 (layer F.Cu) (tedit 53A45415)
    (at 111.887 18.415)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH1 (at 5.969 -1.397) (layer F.SilkS) hide)
    (fp_text value 6-32 (at 0 5.99948) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 -0.254) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
  )
  (module all_fp:Pin_Header_Straight_2x17 (layer F.Cu) (tedit 53990254)
    (at 146.431 148.336)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at 6.985 -5.588) (layer F.SilkS))
    (fp_text value CON34 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -20.32 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole oval (at -20.32 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at -17.78 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 4 thru_hole oval (at -17.78 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at -15.24 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 6 thru_hole oval (at -15.24 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at -12.7 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 8 thru_hole oval (at -12.7 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(J4-Pad8)"))
    (pad 9 thru_hole oval (at -10.16 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 10 thru_hole oval (at -10.16 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J4-Pad10)"))
    (pad 11 thru_hole oval (at -7.62 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 12 thru_hole oval (at -7.62 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J4-Pad12)"))
    (pad 13 thru_hole oval (at -5.08 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 14 thru_hole oval (at -5.08 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J4-Pad14)"))
    (pad 15 thru_hole oval (at -2.54 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 16 thru_hole oval (at -2.54 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 171 RECOVERY_DRIVE2_SEL))
    (pad 17 thru_hole oval (at 0 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 18 thru_hole oval (at 0 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J4-Pad18)"))
    (pad 19 thru_hole oval (at 2.54 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 20 thru_hole oval (at 2.54 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(J4-Pad20)"))
    (pad 21 thru_hole oval (at 5.08 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 22 thru_hole oval (at 5.08 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(J4-Pad22)"))
    (pad 23 thru_hole oval (at 7.62 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 24 thru_hole oval (at 7.62 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(J4-Pad24)"))
    (pad 25 thru_hole oval (at 10.16 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 26 thru_hole oval (at 10.16 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(J4-Pad26)"))
    (pad 27 thru_hole oval (at 12.7 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 28 thru_hole oval (at 12.7 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(J4-Pad28)"))
    (pad 29 thru_hole oval (at 15.24 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 30 thru_hole oval (at 15.24 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(J4-Pad30)"))
    (pad 31 thru_hole oval (at 17.78 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 32 thru_hole oval (at 17.78 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(J4-Pad32)"))
    (pad 33 thru_hole oval (at 20.32 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 34 thru_hole oval (at 20.32 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(J4-Pad34)"))
    (model Pin_Headers/Pin_Header_Straight_2x17.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:sip8 (layer F.Cu) (tedit 5389DE29)
    (at 217.705 100.74 90)
    (fp_text reference RN2 (at 11.303 0.508 180) (layer F.SilkS))
    (fp_text value RN6 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 8.89 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole oval (at 6.35 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /emu/E_STEP))
    (pad 3 thru_hole oval (at 3.81 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /emu/E_SEL1))
    (pad 4 thru_hole oval (at 1.27 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /emu/E_SEL2))
    (pad 5 thru_hole oval (at -1.27 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /emu/E_SEL3))
    (pad 6 thru_hole oval (at -3.81 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /emu/E_SEL4))
    (pad 7 thru_hole oval (at -6.35 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /emu/E_DIR_IN))
    (pad 8 thru_hole oval (at -8.89 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Socket_Strips/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:sip8 (layer F.Cu) (tedit 5389DE33)
    (at 217.094 71.9328 90)
    (fp_text reference RN1 (at 11.303 0.508 180) (layer F.SilkS))
    (fp_text value RN6 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 8.89 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole oval (at 6.35 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /emu/E_HEAD3))
    (pad 3 thru_hole oval (at 3.81 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /emu/E_HEAD2))
    (pad 4 thru_hole oval (at 1.27 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /emu/E_WRITE))
    (pad 5 thru_hole oval (at -1.27 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /emu/E_HEAD0))
    (pad 6 thru_hole oval (at -3.81 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /emu/E_UNUSED))
    (pad 7 thru_hole oval (at -6.35 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /emu/E_HEAD1))
    (pad 8 thru_hole oval (at -8.89 0 270) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Socket_Strips/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:sip8 (layer F.Cu) (tedit 537AB6FA)
    (at 138.684 141.097 180)
    (fp_text reference RN3 (at 11.303 0.508 270) (layer F.SilkS))
    (fp_text value RN6 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 8.89 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole oval (at 6.35 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(J4-Pad8)"))
    (pad 3 thru_hole oval (at 3.81 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J4-Pad10)"))
    (pad 4 thru_hole oval (at 1.27 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J4-Pad12)"))
    (pad 5 thru_hole oval (at -1.27 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(J4-Pad20)"))
    (pad 6 thru_hole oval (at -3.81 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(J4-Pad22)"))
    (pad 7 thru_hole oval (at -6.35 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J3-Pad1)"))
    (pad 8 thru_hole oval (at -8.89 0) (size 1.397 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Socket_Strips/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 53999492)
    (at 214.757 26.67)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at -3.175 0) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(J5-Pad4)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 537AB7EB)
    (at 215.138 42.672)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at -0.08128 -2.58064) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(D1-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 537AB7B8)
    (at 143.891 49.149)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P6 (at -0.127 2.667) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 537AB7B8)
    (at 185.801 96.52)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P5 (at -0.127 2.667) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 179.705 42.418 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference F1 (at 0.0254 2.6162 90) (layer F.SilkS))
    (fp_text value 3A (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 62 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 60 "Net-(C6-Pad1)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53891460)
    (at 203.073 130.556 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R23 (at -0.127 -3.302 270) (layer F.SilkS))
    (fp_text value 100 (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 104 "Net-(J6-Pad13)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 105 "Net-(J6-Pad14)"))
    (model discret/resistors/horizontal/r_h_100R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53990CDC)
    (at 140.589 72.898 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R22 (at 8.382 1.524 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 173 ~MFM1_IN))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53990306)
    (at 157.607 93.98 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R21 (at 0.4445 2.667 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 53 I2C2_SDA))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538914D9)
    (at 161.671 93.98 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R20 (at -0.127 -2.794 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 52 I2C2_SCL))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53990719)
    (at 183.324 33.8455 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R19 (at 2.2225 -2.8575 90) (layer F.SilkS))
    (fp_text value 267 (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 115 "Net-(R19-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 51 GND))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 539902E5)
    (at 165.735 81.534)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R18 (at -1.8415 -2.6035) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 114 "Net-(P4-Pad4)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 165.735 85.09)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R17 (at 0.0254 2.6162) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 113 "Net-(P4-Pad2)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 170.815 103.632 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R16 (at 0.0254 2.6162 180) (layer F.SilkS))
    (fp_text value 732 (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 172 V12_ADC))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 50 AGND))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 539906A2)
    (at 155.702 50.927 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R14 (at 1.905 -3.048 270) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 55 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 63 "Net-(D2-Pad1)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538914BB)
    (at 137.922 47.244 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R12 (at -3.175 -2.794 270) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 59 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 51 GND))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53A64447)
    (at 136.017 29.464 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R11 (at -6.985 2.286 270) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 58 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 59 "Net-(C4-Pad2)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5399031B)
    (at 151.003 29.718 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R10 (at -7.747 1.905 270) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 57 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 58 "Net-(C3-Pad2)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53A44066)
    (at 158.115 41.656 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R9 (at 8.0645 -0.127 180) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 56 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 57 "Net-(C2-Pad2)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53990321)
    (at 166.0525 29.718 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R8 (at 7.239 -2.413 90) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 55 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 56 "Net-(C1-Pad2)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53990207)
    (at 121.793 134.366 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R7 (at 0.3175 -2.6035 90) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 100 "Net-(J4-Pad6)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538914EE)
    (at 136.271 103.124 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R5 (at 8.382 0.254 180) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 49 /emu/~MFM_READ_EN))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53990236)
    (at 178.791 129.896 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at -8.128 0.1905 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 67 "Net-(J1-Pad14)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 66 "Net-(J1-Pad13)"))
    (model discret/resistors/horizontal/r_h_100R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 136.398 98.933 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0.0254 2.6162 180) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 47 /emu/~EMU_EN))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 53990CDF)
    (at 136.779 72.898 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at -0.508 3.048 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 48 /emu/~MFM0_IN))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3.3V))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 212.979 50.038)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R15 (at 0.0254 2.6162) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 172 V12_ADC))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 61 "Net-(D1-Pad1)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44ABC)
    (at 129.286 53.34 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U10 (at 0.4445 5.08 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(C4-Pad2)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 135))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44ABE)
    (at 129.794 35.4965 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U9 (at 0.127 5.2705 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(C4-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(C3-Pad2)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 135))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44ACF)
    (at 144.4625 35.4965 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U8 (at 2.4765 4.445 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(C2-Pad2)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 135))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44AC4)
    (at 157.988 35.4965 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U7 (at 2.0955 4.572 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(C2-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C1-Pad2)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 135))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44AC8)
    (at 172.4025 35.4965 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U6 (at 2.3495 4.7625 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C1-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C1-Pad1)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 135))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 5389DD97)
    (at 208.407 89.662 180)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C18 (at 0.381 2.794 180) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53868C0F)
    (at 165.227 74.422 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C17 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53868C0F)
    (at 125.222 134.366 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C16 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 5399021C)
    (at 129.73 121.984 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C15 (at -0.0635 2.6035 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 5389145B)
    (at 194.945 114.808 180)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C14 (at 4.826 0.508 180) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53868C0F)
    (at 195.453 67.564 180)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C13 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53868C0F)
    (at 208.407 55.626 180)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C12 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53990A55)
    (at 155.829 121.92 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C11 (at 4.699 0.9525 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53990233)
    (at 166.294 136.449 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C10 (at -0.0635 2.667 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 538B4C61)
    (at 186.817 46.228 90)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C9 (at -0.0254 -3.5052 90) (layer F.SilkS))
    (fp_text value "22uF 10V" (at 0 3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 5399046B)
    (at 191.897 46.228 90)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C8 (at 4.826 0 180) (layer F.SilkS))
    (fp_text value "22uF 10V" (at 0 3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 53990472)
    (at 196.977 46.228 90)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C7 (at 0.508 3.81 90) (layer F.SilkS))
    (fp_text value "22uF 10V" (at 0 3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 53990335)
    (at 198.755 37.846 270)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C6 (at 0.381 -4.064 270) (layer F.SilkS))
    (fp_text value "10uF 25V" (at 0 3.556 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:BEAGLEBONEBLACK (layer F.Cu) (tedit 53920633)
    (at 151.003 85.5345 180)
    (tags "beaglebone black")
    (fp_text reference U1 (at 0 1.778 180) (layer F.SilkS) hide)
    (fp_text value BEAGLEBONEBLACK (at 0 -1.143 180) (layer F.SilkS) hide)
    (fp_text user 40 (at -24.892 -20.32 180) (layer F.SilkS))
    (fp_text user 30 (at -12.192 -20.32 180) (layer F.SilkS))
    (fp_text user 20 (at 0.508 -20.32 180) (layer F.SilkS))
    (fp_text user 10 (at 13.462 -20.32 180) (layer F.SilkS))
    (fp_text user 39 (at -24.638 20.574 180) (layer F.SilkS))
    (fp_text user 29 (at -11.938 20.574 180) (layer F.SilkS))
    (fp_text user 19 (at 0.635 20.447 180) (layer F.SilkS))
    (fp_text user 9 (at 13.3096 20.3708 180) (layer F.SilkS))
    (fp_text user J9 (at 26.5176 -19.8628 180) (layer F.SilkS))
    (fp_text user J8 (at 26.7208 19.6596 180) (layer F.SilkS))
    (pad M1 thru_hole circle (at -37.465 -20.955 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad M2 thru_hole circle (at 28.575 -24.13 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad M3 thru_hole circle (at 28.575 24.13 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad M4 thru_hole circle (at -37.465 20.955 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad C1 thru_hole rect (at 23.495 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad C2 thru_hole circle (at 23.495 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad C3 thru_hole circle (at 20.955 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad C4 thru_hole circle (at 20.955 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad C5 thru_hole circle (at 18.415 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad C6 thru_hole circle (at 18.415 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad C7 thru_hole circle (at 15.875 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(U1-PadC7)"))
    (pad C8 thru_hole circle (at 15.875 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(U1-PadC8)"))
    (pad C9 thru_hole circle (at 13.335 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(U1-PadC9)"))
    (pad C10 thru_hole circle (at 13.335 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 143 "Net-(U1-PadC10)"))
    (pad C11 thru_hole circle (at 10.795 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /emu/TRACK0))
    (pad C12 thru_hole circle (at 10.795 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /emu/~EMU_EN))
    (pad C13 thru_hole circle (at 8.255 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /emu/RECOVERY))
    (pad C14 thru_hole circle (at 8.255 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /emu/~MFM_READ_EN))
    (pad C15 thru_hole circle (at 5.715 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 144 "Net-(U1-PadC15)"))
    (pad C16 thru_hole circle (at 5.715 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 145 "Net-(U1-PadC16)"))
    (pad C17 thru_hole circle (at 3.175 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /emu/HEAD3))
    (pad C18 thru_hole circle (at 3.175 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /emu/HEAD2))
    (pad C19 thru_hole circle (at 0.635 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 I2C2_SCL))
    (pad C20 thru_hole circle (at 0.635 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 I2C2_SDA))
    (pad C21 thru_hole circle (at -1.905 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /emu/HEAD1))
    (pad C22 thru_hole circle (at -1.905 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /emu/HEAD0))
    (pad C23 thru_hole circle (at -4.445 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 146 "Net-(U1-PadC23)"))
    (pad C24 thru_hole circle (at -4.445 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /emu/EXPANSION13))
    (pad C25 thru_hole circle (at -6.985 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /emu/STEP))
    (pad C26 thru_hole circle (at -6.985 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /emu/EXPANSION4))
    (pad C27 thru_hole circle (at -9.525 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /emu/INDEX))
    (pad C28 thru_hole circle (at -9.525 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /emu/WFAULT))
    (pad C29 thru_hole circle (at -12.065 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /emu/SELECTED))
    (pad C30 thru_hole circle (at -12.065 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /emu/SEEK_DONE))
    (pad C31 thru_hole circle (at -14.605 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /emu/WRITE))
    (pad C32 thru_hole circle (at -14.605 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 147 "Net-(U1-PadC32)"))
    (pad C33 thru_hole circle (at -17.145 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 148 "Net-(U1-PadC33)"))
    (pad C34 thru_hole circle (at -17.145 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 AGND))
    (pad C35 thru_hole circle (at -19.685 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 149 "Net-(U1-PadC35)"))
    (pad C36 thru_hole circle (at -19.685 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(U1-PadC36)"))
    (pad C37 thru_hole circle (at -22.225 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(U1-PadC37)"))
    (pad C38 thru_hole circle (at -22.225 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(U1-PadC38)"))
    (pad C39 thru_hole circle (at -24.765 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 172 V12_ADC))
    (pad C40 thru_hole circle (at -24.765 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(U1-PadC40)"))
    (pad C41 thru_hole circle (at -27.305 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /emu/DIR_IN))
    (pad C42 thru_hole circle (at -27.305 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /emu/READY))
    (pad C43 thru_hole circle (at -29.845 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad C44 thru_hole circle (at -29.845 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad C45 thru_hole circle (at -32.385 -25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad C46 thru_hole circle (at -32.385 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad B1 thru_hole rect (at 23.495 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad B2 thru_hole circle (at 23.495 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad B3 thru_hole circle (at 20.955 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(U1-PadB3)"))
    (pad B4 thru_hole circle (at 20.955 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(U1-PadB4)"))
    (pad B5 thru_hole circle (at 18.415 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 141 "Net-(U1-PadB5)"))
    (pad B6 thru_hole circle (at 18.415 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 142 "Net-(U1-PadB6)"))
    (pad B7 thru_hole circle (at 15.875 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /emu/EXPANSION6))
    (pad B8 thru_hole circle (at 15.875 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /emu/EXPANSION7))
    (pad B9 thru_hole circle (at 13.335 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /emu/EXPANSION9))
    (pad B10 thru_hole circle (at 13.335 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /emu/EXPANSION8))
    (pad B11 thru_hole circle (at 10.795 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /emu/~MFM0_IN))
    (pad B12 thru_hole circle (at 10.795 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 173 ~MFM1_IN))
    (pad B13 thru_hole circle (at 8.255 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /emu/SEL2))
    (pad B14 thru_hole circle (at 8.255 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /emu/SEL3))
    (pad B15 thru_hole circle (at 5.715 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 MFM_DATA))
    (pad B16 thru_hole circle (at 5.715 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(U1-PadB16)"))
    (pad B17 thru_hole circle (at 3.175 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /emu/SEL4))
    (pad B18 thru_hole circle (at 3.175 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /emu/EXPANSION5))
    (pad B19 thru_hole circle (at 0.635 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /emu/SEL1))
    (pad B20 thru_hole circle (at 0.635 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(U1-PadB20)"))
    (pad B21 thru_hole circle (at -1.905 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(U1-PadB21)"))
    (pad B22 thru_hole circle (at -1.905 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(U1-PadB22)"))
    (pad B23 thru_hole circle (at -4.445 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(U1-PadB23)"))
    (pad B24 thru_hole circle (at -4.445 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(U1-PadB24)"))
    (pad B25 thru_hole circle (at -6.985 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(U1-PadB25)"))
    (pad B26 thru_hole circle (at -6.985 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(U1-PadB26)"))
    (pad B27 thru_hole circle (at -9.525 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /emu/EXPANSION0))
    (pad B28 thru_hole circle (at -9.525 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /emu/EXPANSION2))
    (pad B29 thru_hole circle (at -12.065 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /emu/EXPANSION1))
    (pad B30 thru_hole circle (at -12.065 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /emu/EXPANSION3))
    (pad B31 thru_hole circle (at -14.605 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(U1-PadB31)"))
    (pad B32 thru_hole circle (at -14.605 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 128 "Net-(U1-PadB32)"))
    (pad B33 thru_hole circle (at -17.145 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(U1-PadB33)"))
    (pad B34 thru_hole circle (at -17.145 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 130 "Net-(U1-PadB34)"))
    (pad B35 thru_hole circle (at -19.685 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(U1-PadB35)"))
    (pad B36 thru_hole circle (at -19.685 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(U1-PadB36)"))
    (pad B37 thru_hole circle (at -22.225 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(U1-PadB37)"))
    (pad B38 thru_hole circle (at -22.225 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(U1-PadB38)"))
    (pad B39 thru_hole circle (at -24.765 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(U1-PadB39)"))
    (pad B40 thru_hole circle (at -24.765 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 137 "Net-(U1-PadB40)"))
    (pad B41 thru_hole circle (at -27.305 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 138 "Net-(U1-PadB41)"))
    (pad B42 thru_hole circle (at -27.305 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 139 "Net-(U1-PadB42)"))
    (pad B43 thru_hole circle (at -29.845 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /emu/EXPANSION12))
    (pad B44 thru_hole circle (at -29.845 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 140 "Net-(U1-PadB44)"))
    (pad B45 thru_hole circle (at -32.385 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /emu/EXPANSION10))
    (pad B46 thru_hole circle (at -32.385 25.4 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /emu/EXPANSION11))
    (model /home/djg/mfm/all_fp.pretty/beaglebone_black.wrl
      (at (xyz 1.8 1.08 -0.7))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
    (model Pin_Headers/Pin_Header_Straight_2x23.wrl
      (at (xyz -0.18 -0.95 -0.045))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers/Pin_Header_Straight_2x23.wrl
      (at (xyz -0.18 0.95 -0.045))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module all_fp:LDO03 (layer F.Cu) (tedit 53922E91)
    (at 190.5 37.211)
    (fp_text reference U12 (at 3.175 -14.605) (layer F.SilkS))
    (fp_text value LDO03H (at 0 -2.794) (layer F.SilkS) hide)
    (pad 5 thru_hole oval (at -3.4036 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(R19-Pad1)"))
    (pad 4 thru_hole oval (at -1.7018 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 2 thru_hole oval (at 1.7018 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(C6-Pad1)"))
    (pad 1 thru_hole rect (at 3.4036 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(U12-Pad1)"))
    (pad 6 thru_hole circle (at -0.0762 -12.0142) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(U12-Pad6)"))
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 539996F4)
    (at 158.115 135.128 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R6 (at -2.54 -3.048 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 117 "Net-(R6-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 51 GND))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5398FE3F)
    (at 200.787 105.6 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at 4.064 2.921 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 51 GND))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 116 "Net-(R3-Pad2)"))
    (model discret/resistors/horizontal/r_h_5K6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 53A65005)
    (at 129.413 45.466 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C5 (at 5.08 -3.175 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 1.9812 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 GND))
    (pad 1 thru_hole rect (at 0 3.476 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(C4-Pad2)"))
    (model discret/Capacitor/cp_10x21mm.wrl
      (at (xyz 0 -0.04 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 53A65005)
    (at 172.6565 27.432 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C1 (at 5.08 -3.175 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 1.9812 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 3.476 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C1-Pad1)"))
    (model discret/Capacitor/cp_10x21mm.wrl
      (at (xyz 0 -0.04 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 53A65005)
    (at 157.607 27.686 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C2 (at 5.08 -3.175 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 1.9812 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 3.476 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C1-Pad2)"))
    (model discret/Capacitor/cp_10x21mm.wrl
      (at (xyz 0 -0.04 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 53A65005)
    (at 127.635 27.4955 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C4 (at 5.08 -3.175 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 1.9812 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(C4-Pad2)"))
    (pad 1 thru_hole rect (at 0 3.476 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(C3-Pad2)"))
    (model discret/Capacitor/cp_10x21mm.wrl
      (at (xyz 0 -0.04 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 53A65005)
    (at 142.494 27.6225 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C3 (at 5.08 -3.175 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 1.9812 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(C3-Pad2)"))
    (pad 1 thru_hole rect (at 0 3.476 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(C2-Pad2)"))
    (model discret/Capacitor/cp_10x21mm.wrl
      (at (xyz 0 -0.04 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 144.8054 72.0344 90) (layer F.SilkS))
  (gr_text 3 (at 178.1175 87.503) (layer F.SilkS))
  (gr_text 1 (at 175.387 87.503) (layer F.SilkS))
  (gr_text 34 (at 222.504 104.3686 90) (layer B.SilkS))
  (gr_text 2 (at 222.25 63.8048 90) (layer B.SilkS))
  (gr_text 20 (at 222.504 149.479 90) (layer B.SilkS))
  (gr_text 2 (at 222.504 127 90) (layer B.SilkS))
  (gr_text +5 (at 201.3585 49.0855) (layer F.SilkS))
  (gr_text 1 (at 220.599 149.606 90) (layer F.SilkS))
  (gr_text 20 (at 209.296 126.746 90) (layer F.SilkS))
  (gr_text 20 (at 153.8478 98.5012 90) (layer F.SilkS))
  (gr_text 1 (at 142.5194 76.5556 90) (layer F.SilkS))
  (gr_text 20 (at 200.787 142.875) (layer F.SilkS))
  (gr_text 1 (at 178.308 153.924) (layer F.SilkS))
  (gr_text 34 (at 166.9415 142.875) (layer F.SilkS))
  (gr_text 1 (at 125.73 153.924) (layer F.SilkS))
  (gr_line (start 128.143 91.948) (end 117.475 91.948) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 128.143 74.168) (end 128.143 91.948) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 117.475 74.168) (end 128.143 74.168) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 117.475 74.168) (end 117.475 14.986) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 117.475 161.036) (end 117.475 91.948) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_text GND (at 143.637 46.101) (layer F.SilkS))
  (gr_text GND (at 185.928 93.472) (layer F.SilkS))
  (gr_line (start 222.885 130.937) (end 222.885 130.175) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 222.885 68.072) (end 222.885 67.31) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 14.986) (end 224.155 14.986) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 52.578) (end 234.315 14.986) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 52.578) (end 234.315 52.578) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 61.595) (end 224.155 52.578) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 61.595) (end 224.155 61.595) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 62.357) (end 233.553 61.595) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 67.31) (end 234.315 62.357) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 222.885 67.31) (end 234.315 67.31) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 68.072) (end 222.885 68.072) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 106.045) (end 234.315 68.072) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 106.807) (end 234.315 106.045) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 106.807) (end 233.553 106.807) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 124.46) (end 224.155 106.807) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 124.46) (end 224.155 124.46) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.68 124.587) (end 233.553 124.46) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 125.222) (end 233.68 124.587) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 130.175) (end 234.315 125.222) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 222.885 130.937) (end 234.315 130.937) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 130.175) (end 222.885 130.175) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 151.13) (end 234.315 130.937) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 151.892) (end 234.315 151.13) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 232.791 151.892) (end 233.553 151.892) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 151.892) (end 232.791 151.892) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 161.036) (end 224.155 151.892) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_text 12V (at 215.011 46.101) (layer F.SilkS))
  (gr_text 5V (at 215.138 23.749) (layer F.SilkS))
  (gr_text WRITE (at 121.031 122.936 90) (layer F.SilkS))
  (gr_line (start 117.475 161.036) (end 224.155 161.036) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 224.155 14.986) (end 117.475 14.986) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 51) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.7004 151.5618) (xy 218.4654 151.511) (xy 218.4654 141.5034) (xy 221.869 141.5034) (xy 221.8944 155.3718)
        (xy 203.962 155.3718) (xy 201.7522 154.9146) (xy 200.6346 154.94) (xy 198.8058 155.2956) (xy 193.7004 155.2956)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.569 106.807) (xy 223.901 106.807) (xy 223.901 61.595) (xy 234.569 61.595)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.901 61.595) (xy 223.901 106.807) (xy 234.569 106.807) (xy 234.569 61.595) (xy 223.9645 61.595)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.569 151.892) (xy 223.901 151.892) (xy 223.901 124.46) (xy 234.569 124.46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.569 151.892) (xy 223.901 151.892) (xy 223.901 124.46) (xy 234.569 124.46)
      )
    )
  )
)
