(module LEDs:LED-5MM (layer F.Cu)
  (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
  (tags "LED led 5mm 5MM 100mil 2,54mm")
  (fp_text reference D2 (at -3.302 3.683 90) (layer F.SilkS))
  (fp_text value LED (at 0 3.81) (layer F.SilkS) hide)
  (pad 1 thru_hole circle (at -1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
  (model discret/leds/led5_vertical_verde.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
