(kicad_pcb (version 4) (host pcbnew "(after 2015-mar-04 BZR unknown)-product")
  (general
    (links 395)
    (no_connects 0)
    (area 117.424199 14.935199 234.365801 161.086801)
    (thickness 1.6)
    (drawings 65)
    (tracks 2007)
    (zones 0)
    (modules 90)
    (nets 110)
  )
  (page USLetter)
  (title_block
    (title "MFM Disk Reader and Emulator")
    (date "18 May 2014")
    (rev 1)
    (company "David Gesswein")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.143)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.254)
    (segment_width 0.2032)
    (edge_width 0.1016)
    (via_size 0.889)
    (via_drill 0.508)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.254)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.254)
    (pad_size 2.2352 2.2352)
    (pad_drill 1.0668)
    (pad_to_mask_clearance 0.1016)
    (solder_mask_min_width 0.0762)
    (aux_axis_origin 0 0)
    (grid_origin 97.155 15.24)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /emu/DIR_IN)
  (net 3 /emu/EXPANSION0)
  (net 4 /emu/EXPANSION1)
  (net 5 /emu/EXPANSION10)
  (net 6 /emu/EXPANSION11)
  (net 7 /emu/EXPANSION12)
  (net 8 /emu/EXPANSION2)
  (net 9 /emu/EXPANSION3)
  (net 10 /emu/EXPANSION4)
  (net 11 /emu/EXPANSION5)
  (net 12 /emu/EXPANSION6)
  (net 13 /emu/EXPANSION7)
  (net 14 /emu/EXPANSION8)
  (net 15 /emu/EXPANSION9)
  (net 16 /emu/E_DIR_IN)
  (net 17 /emu/E_HEAD0)
  (net 18 /emu/E_HEAD1)
  (net 19 /emu/E_HEAD2)
  (net 20 /emu/E_HEAD3)
  (net 21 /emu/E_SEL1)
  (net 22 /emu/E_SEL2)
  (net 23 /emu/E_SEL3)
  (net 24 /emu/E_SEL4)
  (net 25 /emu/E_STEP)
  (net 26 /emu/E_WRITE)
  (net 27 /emu/HEAD0)
  (net 28 /emu/HEAD1)
  (net 29 /emu/HEAD2)
  (net 30 /emu/HEAD3)
  (net 31 /emu/INDEX)
  (net 32 /emu/READY)
  (net 33 /emu/RECOVERY)
  (net 34 /emu/SEEK_DONE)
  (net 35 /emu/SEL1)
  (net 36 /emu/SEL3)
  (net 37 /emu/SEL4)
  (net 38 /emu/SELECTED)
  (net 39 /emu/STEP)
  (net 40 /emu/TRACK0)
  (net 41 /emu/WFAULT)
  (net 42 /emu/WRITE)
  (net 43 /emu/~EMU_EN)
  (net 44 /emu/~MFM0_IN)
  (net 45 /emu/~MFM_READ_EN)
  (net 46 AGND)
  (net 47 GND)
  (net 48 I2C2_SCL)
  (net 49 I2C2_SDA)
  (net 50 MFM_DATA)
  (net 51 "Net-(C1-Pad1)")
  (net 52 "Net-(C1-Pad2)")
  (net 53 "Net-(C2-Pad2)")
  (net 54 "Net-(C3-Pad2)")
  (net 55 "Net-(C4-Pad2)")
  (net 56 "Net-(C6-Pad1)")
  (net 57 "Net-(D1-Pad1)")
  (net 58 "Net-(D1-Pad2)")
  (net 59 "Net-(D2-Pad1)")
  (net 60 "Net-(J1-Pad1)")
  (net 61 "Net-(J1-Pad13)")
  (net 62 "Net-(J1-Pad14)")
  (net 63 "Net-(J1-Pad17)")
  (net 64 "Net-(J1-Pad18)")
  (net 65 "Net-(J2-Pad10)")
  (net 66 "Net-(J2-Pad12)")
  (net 67 "Net-(J2-Pad20)")
  (net 68 "Net-(J2-Pad22)")
  (net 69 "Net-(J2-Pad8)")
  (net 70 "Net-(J3-Pad1)")
  (net 71 "Net-(J4-Pad10)")
  (net 72 "Net-(J4-Pad12)")
  (net 73 "Net-(J4-Pad14)")
  (net 74 "Net-(J4-Pad18)")
  (net 75 "Net-(J4-Pad2)")
  (net 76 "Net-(J4-Pad20)")
  (net 77 "Net-(J4-Pad22)")
  (net 78 "Net-(J4-Pad24)")
  (net 79 "Net-(J4-Pad26)")
  (net 80 "Net-(J4-Pad28)")
  (net 81 "Net-(J4-Pad30)")
  (net 82 "Net-(J4-Pad32)")
  (net 83 "Net-(J4-Pad34)")
  (net 84 "Net-(J4-Pad4)")
  (net 85 "Net-(J4-Pad6)")
  (net 86 "Net-(J4-Pad8)")
  (net 87 "Net-(J5-Pad4)")
  (net 88 "Net-(J6-Pad13)")
  (net 89 "Net-(J6-Pad14)")
  (net 90 "Net-(J6-Pad17)")
  (net 91 "Net-(J6-Pad18)")
  (net 92 "Net-(P1-Pad1)")
  (net 93 "Net-(P4-Pad2)")
  (net 94 "Net-(P4-Pad4)")
  (net 95 "Net-(R19-Pad1)")
  (net 96 RECOVERY_DRIVE2_SEL)
  (net 97 V12_ADC)
  (net 98 ~MFM1_IN)
  (net 99 /emu/INT_SEL1)
  (net 100 INT_SEL2)
  (net 101 "Net-(P9-Pad2)")
  (net 102 +3V3)
  (net 103 SEL2)
  (net 104 "Net-(R24-Pad2)")
  (net 105 "Net-(R26-Pad1)")
  (net 106 "Net-(RN2-Pad10)")
  (net 107 POWER_BUTTON)
  (net 108 "Net-(R6-Pad2)")
  (net 109 /emu/EXPANSION13)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net /emu/DIR_IN)
    (add_net /emu/EXPANSION0)
    (add_net /emu/EXPANSION1)
    (add_net /emu/EXPANSION10)
    (add_net /emu/EXPANSION11)
    (add_net /emu/EXPANSION12)
    (add_net /emu/EXPANSION13)
    (add_net /emu/EXPANSION2)
    (add_net /emu/EXPANSION3)
    (add_net /emu/EXPANSION4)
    (add_net /emu/EXPANSION5)
    (add_net /emu/EXPANSION6)
    (add_net /emu/EXPANSION7)
    (add_net /emu/EXPANSION8)
    (add_net /emu/EXPANSION9)
    (add_net /emu/E_DIR_IN)
    (add_net /emu/E_HEAD0)
    (add_net /emu/E_HEAD1)
    (add_net /emu/E_HEAD2)
    (add_net /emu/E_HEAD3)
    (add_net /emu/E_SEL1)
    (add_net /emu/E_SEL2)
    (add_net /emu/E_SEL3)
    (add_net /emu/E_SEL4)
    (add_net /emu/E_STEP)
    (add_net /emu/E_WRITE)
    (add_net /emu/HEAD0)
    (add_net /emu/HEAD1)
    (add_net /emu/HEAD2)
    (add_net /emu/HEAD3)
    (add_net /emu/INDEX)
    (add_net /emu/INT_SEL1)
    (add_net /emu/READY)
    (add_net /emu/RECOVERY)
    (add_net /emu/SEEK_DONE)
    (add_net /emu/SEL1)
    (add_net /emu/SEL3)
    (add_net /emu/SEL4)
    (add_net /emu/SELECTED)
    (add_net /emu/STEP)
    (add_net /emu/TRACK0)
    (add_net /emu/WFAULT)
    (add_net /emu/WRITE)
    (add_net /emu/~EMU_EN)
    (add_net /emu/~MFM0_IN)
    (add_net /emu/~MFM_READ_EN)
    (add_net AGND)
    (add_net GND)
    (add_net I2C2_SCL)
    (add_net I2C2_SDA)
    (add_net INT_SEL2)
    (add_net MFM_DATA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J4-Pad18)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad20)")
    (add_net "Net-(J4-Pad22)")
    (add_net "Net-(J4-Pad24)")
    (add_net "Net-(J4-Pad26)")
    (add_net "Net-(J4-Pad28)")
    (add_net "Net-(J4-Pad30)")
    (add_net "Net-(J4-Pad32)")
    (add_net "Net-(J4-Pad34)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J6-Pad13)")
    (add_net "Net-(J6-Pad14)")
    (add_net "Net-(J6-Pad17)")
    (add_net "Net-(J6-Pad18)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(RN2-Pad10)")
    (add_net POWER_BUTTON)
    (add_net RECOVERY_DRIVE2_SEL)
    (add_net SEL2)
    (add_net V12_ADC)
    (add_net ~MFM1_IN)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 1.27)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44ABC)
    (at 149.479 38.1 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U8 (at 0.4445 5.08 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C2-Pad2)"))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 558E0979)
    (at 176.657 83.566)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P4 (at 4.826 0.254) (layer F.SilkS))
    (fp_text value CONN_2X2 (at -0.549409 4.1672) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole oval (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 4 thru_hole oval (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(P4-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 558E094F)
    (at 214.503 95.504)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 1.143 10.795) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 0 -3.1) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 99 /emu/INT_SEL1))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 21 /emu/E_SEL1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 99 /emu/INT_SEL1))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 22 /emu/E_SEL2))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 99 /emu/INT_SEL1))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 23 /emu/E_SEL3))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 99 /emu/INT_SEL1))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 24 /emu/E_SEL4))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 558E090A)
    (at 203.835 95.504)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 1.397 10.668) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 0 -3.1) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 100 INT_SEL2))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 21 /emu/E_SEL1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 100 INT_SEL2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 22 /emu/E_SEL2))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 100 INT_SEL2))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 23 /emu/E_SEL3))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 100 INT_SEL2))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 24 /emu/E_SEL4))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module all_fp:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 558E08E8)
    (at 147.955 86.36 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J7 (at -0.635 5.715 270) (layer F.SilkS))
    (fp_text value CONN_20 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole oval (at -11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 3 thru_hole oval (at -8.89 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 11 /emu/EXPANSION5))
    (pad 4 thru_hole oval (at -8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 3 /emu/EXPANSION0))
    (pad 5 thru_hole oval (at -6.35 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 15 /emu/EXPANSION9))
    (pad 6 thru_hole oval (at -6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 4 /emu/EXPANSION1))
    (pad 7 thru_hole oval (at -3.81 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 14 /emu/EXPANSION8))
    (pad 8 thru_hole oval (at -3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 9 /emu/EXPANSION3))
    (pad 9 thru_hole oval (at -1.27 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 12 /emu/EXPANSION6))
    (pad 10 thru_hole oval (at -1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 109 /emu/EXPANSION13))
    (pad 11 thru_hole oval (at 1.27 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 13 /emu/EXPANSION7))
    (pad 12 thru_hole oval (at 1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 8 /emu/EXPANSION2))
    (pad 13 thru_hole oval (at 3.81 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 6 /emu/EXPANSION11))
    (pad 14 thru_hole oval (at 3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 5 /emu/EXPANSION10))
    (pad 15 thru_hole oval (at 6.35 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 7 /emu/EXPANSION12))
    (pad 16 thru_hole oval (at 6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 10 /emu/EXPANSION4))
    (pad 17 thru_hole oval (at 8.89 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 18 thru_hole oval (at 8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 19 thru_hole oval (at 11.43 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 48 I2C2_SCL))
    (pad 20 thru_hole oval (at 11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 49 I2C2_SDA))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 558E08BE)
    (at 212.725 140.97 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at 0 -5.715 270) (layer F.SilkS))
    (fp_text value ECON20 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 96 RECOVERY_DRIVE2_SEL))
    (pad 2 thru_hole oval (at -11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 3 thru_hole oval (at -8.89 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at -8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 5 thru_hole oval (at -6.35 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at -6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 7 thru_hole oval (at -3.81 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at -3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 9 thru_hole oval (at -1.27 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at -1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 1.27 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 12 thru_hole oval (at 1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 13 thru_hole oval (at 3.81 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J6-Pad13)"))
    (pad 14 thru_hole oval (at 3.81 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J6-Pad14)"))
    (pad 15 thru_hole oval (at 6.35 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 16 thru_hole oval (at 6.35 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 17 thru_hole oval (at 8.89 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(J6-Pad17)"))
    (pad 18 thru_hole oval (at 8.89 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(J6-Pad18)"))
    (pad 19 thru_hole oval (at 11.43 1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 20 thru_hole oval (at 11.43 -1.27 270) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 558E0893)
    (at 189.611 148.336)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at -1.651 5.588) (layer F.SilkS))
    (fp_text value CON20 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at -11.43 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 3 thru_hole oval (at -8.89 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at -8.89 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 5 thru_hole oval (at -6.35 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at -6.35 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 7 thru_hole oval (at -3.81 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at -3.81 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 9 thru_hole oval (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 12 thru_hole oval (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 13 thru_hole oval (at 3.81 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(J1-Pad17)"))
    (pad 14 thru_hole oval (at 3.81 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(J1-Pad18)"))
    (pad 15 thru_hole oval (at 6.35 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 16 thru_hole oval (at 6.35 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 17 thru_hole oval (at 8.89 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(J1-Pad13)"))
    (pad 18 thru_hole oval (at 8.89 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(J1-Pad14)"))
    (pad 19 thru_hole oval (at 11.43 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 20 thru_hole oval (at 11.43 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_2x17 (layer F.Cu) (tedit 558E086C)
    (at 146.431 148.336)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at -0.381 5.842) (layer F.SilkS))
    (fp_text value CON34 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -20.32 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole oval (at -20.32 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at -17.78 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 4 thru_hole oval (at -17.78 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at -15.24 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 6 thru_hole oval (at -15.24 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at -12.7 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 8 thru_hole oval (at -12.7 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J4-Pad8)"))
    (pad 9 thru_hole oval (at -10.16 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 10 thru_hole oval (at -10.16 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J4-Pad10)"))
    (pad 11 thru_hole oval (at -7.62 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 12 thru_hole oval (at -7.62 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J4-Pad12)"))
    (pad 13 thru_hole oval (at -5.08 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 14 thru_hole oval (at -5.08 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J4-Pad14)"))
    (pad 15 thru_hole oval (at -2.54 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 16 thru_hole oval (at -2.54 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 96 RECOVERY_DRIVE2_SEL))
    (pad 17 thru_hole oval (at 0 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 18 thru_hole oval (at 0 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J4-Pad18)"))
    (pad 19 thru_hole oval (at 2.54 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 20 thru_hole oval (at 2.54 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J4-Pad20)"))
    (pad 21 thru_hole oval (at 5.08 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 22 thru_hole oval (at 5.08 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J4-Pad22)"))
    (pad 23 thru_hole oval (at 7.62 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 24 thru_hole oval (at 7.62 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J4-Pad24)"))
    (pad 25 thru_hole oval (at 10.16 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 26 thru_hole oval (at 10.16 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(J4-Pad26)"))
    (pad 27 thru_hole oval (at 12.7 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 28 thru_hole oval (at 12.7 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J4-Pad28)"))
    (pad 29 thru_hole oval (at 15.24 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 30 thru_hole oval (at 15.24 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J4-Pad30)"))
    (pad 31 thru_hole oval (at 17.78 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 32 thru_hole oval (at 17.78 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J4-Pad32)"))
    (pad 33 thru_hole oval (at 20.32 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 34 thru_hole oval (at 20.32 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J4-Pad34)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x17.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:BEAGLEBONEBLACK (layer F.Cu) (tedit 558E0847)
    (at 151.13 87.63 180)
    (tags "beaglebone black")
    (fp_text reference U1 (at 0 1.778 180) (layer F.SilkS) hide)
    (fp_text value BEAGLEBONEBLACK (at 0 -1.143 180) (layer F.SilkS) hide)
    (fp_text user 40 (at -24.892 -20.32 180) (layer F.SilkS))
    (fp_text user 30 (at -12.192 -20.32 180) (layer F.SilkS))
    (fp_text user 20 (at 0.508 -20.32 180) (layer F.SilkS))
    (fp_text user 10 (at 13.462 -20.32 180) (layer F.SilkS))
    (fp_text user 39 (at -24.638 20.574 180) (layer F.SilkS))
    (fp_text user 29 (at -11.938 20.574 180) (layer F.SilkS))
    (fp_text user 19 (at 0.635 20.447 180) (layer F.SilkS))
    (fp_text user 9 (at 13.3096 20.3708 180) (layer F.SilkS))
    (fp_text user J9 (at 26.5176 -19.8628 180) (layer F.SilkS))
    (fp_text user J8 (at 26.7208 19.6596 180) (layer F.SilkS))
    (pad M1 thru_hole circle (at -37.465 -20.955 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad M2 thru_hole circle (at 28.575 -24.13 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad M3 thru_hole circle (at 28.575 24.13 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad M4 thru_hole circle (at -37.465 20.955 180) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad C1 thru_hole rect (at 23.495 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad C2 thru_hole circle (at 23.495 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad C3 thru_hole circle (at 20.955 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad C4 thru_hole circle (at 20.955 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad C5 thru_hole circle (at 18.415 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad C6 thru_hole circle (at 18.415 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad C7 thru_hole circle (at 15.875 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C8 thru_hole circle (at 15.875 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C9 thru_hole circle (at 13.335 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 107 POWER_BUTTON))
    (pad C10 thru_hole circle (at 13.335 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C11 thru_hole circle (at 10.795 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 40 /emu/TRACK0))
    (pad C12 thru_hole circle (at 10.795 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 43 /emu/~EMU_EN))
    (pad C13 thru_hole circle (at 8.255 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 33 /emu/RECOVERY))
    (pad C14 thru_hole circle (at 8.255 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 45 /emu/~MFM_READ_EN))
    (pad C15 thru_hole circle (at 5.715 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C16 thru_hole circle (at 5.715 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C17 thru_hole circle (at 3.175 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 7 /emu/EXPANSION12))
    (pad C18 thru_hole circle (at 3.175 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 6 /emu/EXPANSION11))
    (pad C19 thru_hole circle (at 0.635 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 48 I2C2_SCL))
    (pad C20 thru_hole circle (at 0.635 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 49 I2C2_SDA))
    (pad C21 thru_hole circle (at -1.905 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 9 /emu/EXPANSION3))
    (pad C22 thru_hole circle (at -1.905 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 8 /emu/EXPANSION2))
    (pad C23 thru_hole circle (at -4.445 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C24 thru_hole circle (at -4.445 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 109 /emu/EXPANSION13))
    (pad C25 thru_hole circle (at -6.985 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 39 /emu/STEP))
    (pad C26 thru_hole circle (at -6.985 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 10 /emu/EXPANSION4))
    (pad C27 thru_hole circle (at -9.525 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 31 /emu/INDEX))
    (pad C28 thru_hole circle (at -9.525 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 41 /emu/WFAULT))
    (pad C29 thru_hole circle (at -12.065 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 38 /emu/SELECTED))
    (pad C30 thru_hole circle (at -12.065 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 34 /emu/SEEK_DONE))
    (pad C31 thru_hole circle (at -14.605 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 42 /emu/WRITE))
    (pad C32 thru_hole circle (at -14.605 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C33 thru_hole circle (at -17.145 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C34 thru_hole circle (at -17.145 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 46 AGND))
    (pad C35 thru_hole circle (at -19.685 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C36 thru_hole circle (at -19.685 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C37 thru_hole circle (at -22.225 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C38 thru_hole circle (at -22.225 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C39 thru_hole circle (at -24.765 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 97 V12_ADC))
    (pad C40 thru_hole circle (at -24.765 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad C41 thru_hole circle (at -27.305 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 2 /emu/DIR_IN))
    (pad C42 thru_hole circle (at -27.305 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 32 /emu/READY))
    (pad C43 thru_hole circle (at -29.845 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad C44 thru_hole circle (at -29.845 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad C45 thru_hole circle (at -32.385 -25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad C46 thru_hole circle (at -32.385 -22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad B1 thru_hole rect (at 23.495 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad B2 thru_hole circle (at 23.495 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad B3 thru_hole circle (at 20.955 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B4 thru_hole circle (at 20.955 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B5 thru_hole circle (at 18.415 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B6 thru_hole circle (at 18.415 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B7 thru_hole circle (at 15.875 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 12 /emu/EXPANSION6))
    (pad B8 thru_hole circle (at 15.875 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 13 /emu/EXPANSION7))
    (pad B9 thru_hole circle (at 13.335 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 15 /emu/EXPANSION9))
    (pad B10 thru_hole circle (at 13.335 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 14 /emu/EXPANSION8))
    (pad B11 thru_hole circle (at 10.795 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 44 /emu/~MFM0_IN))
    (pad B12 thru_hole circle (at 10.795 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 98 ~MFM1_IN))
    (pad B13 thru_hole circle (at 8.255 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 103 SEL2))
    (pad B14 thru_hole circle (at 8.255 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 36 /emu/SEL3))
    (pad B15 thru_hole circle (at 5.715 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 50 MFM_DATA))
    (pad B16 thru_hole circle (at 5.715 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad B17 thru_hole circle (at 3.175 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 37 /emu/SEL4))
    (pad B18 thru_hole circle (at 3.175 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 11 /emu/EXPANSION5))
    (pad B19 thru_hole circle (at 0.635 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 35 /emu/SEL1))
    (pad B20 thru_hole circle (at 0.635 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B21 thru_hole circle (at -1.905 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B22 thru_hole circle (at -1.905 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B23 thru_hole circle (at -4.445 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B24 thru_hole circle (at -4.445 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B25 thru_hole circle (at -6.985 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B26 thru_hole circle (at -6.985 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B27 thru_hole circle (at -9.525 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 3 /emu/EXPANSION0))
    (pad B28 thru_hole circle (at -9.525 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B29 thru_hole circle (at -12.065 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 4 /emu/EXPANSION1))
    (pad B30 thru_hole circle (at -12.065 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B31 thru_hole circle (at -14.605 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 29 /emu/HEAD2))
    (pad B32 thru_hole circle (at -14.605 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 30 /emu/HEAD3))
    (pad B33 thru_hole circle (at -17.145 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 28 /emu/HEAD1))
    (pad B34 thru_hole circle (at -17.145 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B35 thru_hole circle (at -19.685 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 27 /emu/HEAD0))
    (pad B36 thru_hole circle (at -19.685 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B37 thru_hole circle (at -22.225 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B38 thru_hole circle (at -22.225 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B39 thru_hole circle (at -24.765 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B40 thru_hole circle (at -24.765 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B41 thru_hole circle (at -27.305 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B42 thru_hole circle (at -27.305 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B43 thru_hole circle (at -29.845 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B44 thru_hole circle (at -29.845 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (pad B45 thru_hole circle (at -32.385 22.86 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 5 /emu/EXPANSION10))
    (pad B46 thru_hole circle (at -32.385 25.4 180) (size 1.7272 1.7272) (drill 1.0668) (layers *.Cu *.Mask F.SilkS))
    (model ${KIPRJMOD}/all_fp.pretty/beaglebone_black.wrl
      (at (xyz 1.8 1.08 -0.7))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 180))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x23.wrl
      (at (xyz -0.18 -0.95 -0.045))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x23.wrl
      (at (xyz -0.18 0.95 -0.045))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10 (layer F.Cu) (tedit 558E0825)
    (at 145.415 140.335)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference RN2 (at -4.445 0) (layer F.SilkS))
    (fp_text value RN9 (at 0 -3.1) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J4-Pad8)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J4-Pad10)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J4-Pad12)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J4-Pad20)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J4-Pad22)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J3-Pad1)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 INT_SEL2))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 /emu/INT_SEL1))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(RN2-Pad10)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x10.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10 (layer F.Cu) (tedit 558E07F7)
    (at 216.535 62.865 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference RN1 (at -3.937 -0.508 270) (layer F.SilkS))
    (fp_text value RN9 (at 0 -3.1 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /emu/E_HEAD3))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /emu/E_HEAD2))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /emu/E_WRITE))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /emu/E_HEAD0))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /emu/E_HEAD1))
    (pad 9 thru_hole oval (at 20.32 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /emu/E_STEP))
    (pad 10 thru_hole oval (at 22.86 0 270) (size 1.7272 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /emu/E_DIR_IN))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x10.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 558DF3F0)
    (at 200.787 136.144 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U13 (at -5.0292 -5.715 90) (layer F.SilkS))
    (fp_text value MAX3491 (at 0 5.375 90) (layer Dwgs.User) hide)
    (pad 1 smd rect (at -2.9 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.9 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 MFM_DATA))
    (pad 3 smd rect (at -2.9 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 ~MFM1_IN))
    (pad 4 smd rect (at -2.9 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 ~MFM1_IN))
    (pad 5 smd rect (at -2.9 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 MFM_DATA))
    (pad 6 smd rect (at -2.9 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 GND) (thermal_width 0.2794) (thermal_gap 0.508))
    (pad 7 smd rect (at -2.9 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 GND) (zone_connect 1) (thermal_width 0.2794) (thermal_gap 0.508))
    (pad 8 smd rect (at 2.9 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.9 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(J6-Pad17)"))
    (pad 10 smd rect (at 2.9 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(J6-Pad18)"))
    (pad 11 smd rect (at 2.9 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(J6-Pad14)"))
    (pad 12 smd rect (at 2.9 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(J6-Pad13)"))
    (pad 13 smd rect (at 2.9 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 +3V3))
    (pad 14 smd rect (at 2.9 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 558DF492)
    (at 185.039 136.144 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at -4.064 -5.461 90) (layer F.SilkS))
    (fp_text value MAX3491 (at 0 5.375 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.9 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (zone_connect 1) (thermal_width 0.028) (thermal_gap 0.05))
    (pad 2 smd rect (at -2.9 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 MFM_DATA))
    (pad 3 smd rect (at -2.9 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /emu/~MFM0_IN))
    (pad 4 smd rect (at -2.9 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /emu/~MFM0_IN))
    (pad 5 smd rect (at -2.9 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 MFM_DATA))
    (pad 6 smd rect (at -2.9 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 GND) (thermal_width 0.2794) (thermal_gap 0.508))
    (pad 7 smd rect (at -2.9 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 GND) (thermal_width 0.2794) (thermal_gap 0.508))
    (pad 8 smd rect (at 2.9 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.9 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J1-Pad17)"))
    (pad 10 smd rect (at 2.9 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(J1-Pad18)"))
    (pad 11 smd rect (at 2.9 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J1-Pad14)"))
    (pad 12 smd rect (at 2.9 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J1-Pad13)"))
    (pad 13 smd rect (at 2.9 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 +3V3))
    (pad 14 smd rect (at 2.9 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-20__300 (layer F.Cu) (tedit 5389143C)
    (at 156.845 133.35)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U5 (at -13.97 -4.572 90) (layer F.SilkS))
    (fp_text value 74LVC245 (at 6.35 1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J4-Pad8)"))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J4-Pad10)"))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J4-Pad12)"))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J4-Pad20)"))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J4-Pad22)"))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J3-Pad1)"))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(RN2-Pad10)"))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(RN2-Pad10)"))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(RN2-Pad10)"))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(RN2-Pad10)"))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /emu/SELECTED))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /emu/READY))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /emu/INDEX))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /emu/WFAULT))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /emu/TRACK0))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /emu/SEEK_DONE))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /emu/~MFM_READ_EN))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (model Sockets_DIP.3dshapes/DIP-20__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:ECON34 (layer F.Cu) (tedit 55BAD6A9)
    (at 222.885 82.8802 90)
    (fp_text reference J2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value ECON34 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user 33 (at -21.5138 -0.6096 90) (layer F.SilkS))
    (fp_text user 1 (at 18.8468 -0.7112 90) (layer F.SilkS))
    (pad 1 connect rect (at 18.9992 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 2 connect rect (at 18.9992 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 20 /emu/E_HEAD3))
    (pad 3 connect rect (at 16.4592 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 4 connect rect (at 16.4592 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 19 /emu/E_HEAD2))
    (pad 5 connect rect (at 13.9192 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 6 connect rect (at 13.9192 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 26 /emu/E_WRITE))
    (pad 7 connect rect (at 11.3792 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 8 connect rect (at 11.3792 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 69 "Net-(J2-Pad8)"))
    (pad 9 connect rect (at 8.8392 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 10 connect rect (at 8.8392 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 65 "Net-(J2-Pad10)"))
    (pad 11 connect rect (at 6.2992 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 12 connect rect (at 6.2992 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 66 "Net-(J2-Pad12)"))
    (pad 13 connect rect (at 3.7592 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 14 connect rect (at 3.7592 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 17 /emu/E_HEAD0))
    (pad 15 connect rect (at 1.2192 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 16 connect rect (at 1.2192 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask))
    (pad 17 connect rect (at -1.3208 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 18 connect rect (at -1.3208 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 18 /emu/E_HEAD1))
    (pad 19 connect rect (at -3.8608 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 20 connect rect (at -3.8608 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 67 "Net-(J2-Pad20)"))
    (pad 21 connect rect (at -6.4008 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 22 connect rect (at -6.4008 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 68 "Net-(J2-Pad22)"))
    (pad 23 connect rect (at -8.9408 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 24 connect rect (at -8.9408 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 25 /emu/E_STEP))
    (pad 25 connect rect (at -11.4808 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 26 connect rect (at -11.4808 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 21 /emu/E_SEL1))
    (pad 27 connect rect (at -14.0208 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 28 connect rect (at -14.0208 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 22 /emu/E_SEL2))
    (pad 29 connect rect (at -16.5608 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 30 connect rect (at -16.5608 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 23 /emu/E_SEL3))
    (pad 31 connect rect (at -19.1008 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 32 connect rect (at -19.1008 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 24 /emu/E_SEL4))
    (pad 33 connect rect (at -21.6408 6.35 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 34 connect rect (at -21.6408 6.35 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 16 /emu/E_DIR_IN))
  )
  (module all_fp:econ20 (layer F.Cu) (tedit 55BAD805)
    (at 228.981 136.804 90)
    (fp_text reference J1 (at -0.3814 -6.8072 90) (layer F.SilkS))
    (fp_text value ECON20 (at -5.08 0 90) (layer F.SilkS) hide)
    (fp_text user 19 (at -12.7 -6.477 90) (layer F.SilkS))
    (fp_text user 1 (at 9.8929 -6.7437 90) (layer F.SilkS))
    (pad 1 connect rect (at 10.0584 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 60 "Net-(J1-Pad1)"))
    (pad 2 connect rect (at 10.0584 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 47 GND))
    (pad 3 connect rect (at 7.5184 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask))
    (pad 4 connect rect (at 7.5184 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 47 GND))
    (pad 5 connect rect (at 4.9784 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask))
    (pad 6 connect rect (at 4.9784 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 47 GND))
    (pad 7 connect rect (at 2.4384 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask))
    (pad 8 connect rect (at 2.4384 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 47 GND))
    (pad 9 connect rect (at -0.1016 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask))
    (pad 10 connect rect (at -0.1016 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask))
    (pad 11 connect rect (at -2.6416 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 12 connect rect (at -2.6416 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 47 GND))
    (pad 13 connect rect (at -5.1816 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 61 "Net-(J1-Pad13)"))
    (pad 14 connect rect (at -5.1816 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 62 "Net-(J1-Pad14)"))
    (pad 15 connect rect (at -7.7216 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 16 connect rect (at -7.7216 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 47 GND))
    (pad 17 connect rect (at -10.2616 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 63 "Net-(J1-Pad17)"))
    (pad 18 connect rect (at -10.2616 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 64 "Net-(J1-Pad18)"))
    (pad 19 connect rect (at -12.8016 0.254 270) (size 1.524 10.16) (layers F.Cu F.Mask)
      (net 47 GND))
    (pad 20 connect rect (at -12.8016 0.254 270) (size 1.524 10.16) (layers B.Cu B.Mask)
      (net 47 GND))
  )
  (module all_fp:DRVPWR (layer F.Cu) (tedit 55710730)
    (at 215.138 34.544 270)
    (fp_text reference J5 (at -1.905 -1.3335 270) (layer F.SilkS))
    (fp_text value CONN_4 (at -1.27 -10.16 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 6.35 -5.08 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -5.08 270) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 3 thru_hole circle (at -3.81 -5.08 270) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 4 thru_hole circle (at -8.89 -5.08 270) (size 2.794 2.794) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J5-Pad4)"))
    (pad "" np_thru_hole circle (at -6.35 -15.24 270) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 3.81 -15.24 270) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -11.43 -7.62 270) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 8.89 -7.62 270) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (model ${KIPRJMOD}/all_fp.pretty/DRVPWR.wrl
      (at (xyz -0.05 0.21 0.185))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz -90 0 180))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 539906A0)
    (at 133.35 52.07 90)
    (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 5mm 5MM 100mil 2,54mm")
    (fp_text reference D2 (at 4.191 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM20mm (layer F.Cu) (tedit 558E072F)
    (at 188.087 53.848 180)
    (descr "Resistor, Axial, RM 20mm,")
    (tags "Resistor, Axial, RM 20mm,")
    (fp_text reference R13 (at -0.381 -4.064 180) (layer F.SilkS))
    (fp_text value 8.2 (at 0 5.00126 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -9.99998 0 180) (size 1.99898 1.99898) (drill 1.0668) (layers *.Cu *.SilkS *.Mask)
      (net 101 "Net-(P9-Pad2)"))
    (pad 2 thru_hole circle (at 10.32002 0 180) (size 1.99898 1.99898) (drill 1.0668) (layers *.Cu *.SilkS *.Mask)
      (net 51 "Net-(C1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-201AD_Horizontal_RM15 (layer F.Cu) (tedit 53A44BDD)
    (at 208.915 36.195 270)
    (descr "Diode DO-201AD Horizontal")
    (tags "Diode DO-201AD Horizontal SB320 SB340 SB360")
    (fp_text reference D1 (at 0.5715 -4.318 270) (layer F.SilkS))
    (fp_text value 1N5820 (at 0.508 -4.826 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -7.62 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(D1-Pad1)"))
    (pad 2 thru_hole rect (at 7.62 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(D1-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-201AD_Horizontal_RM15 (layer F.Cu) (tedit 537805D4)
    (at 165.544 55.753)
    (descr "Diode DO-201AD Horizontal")
    (tags "Diode DO-201AD Horizontal SB320 SB340 SB360")
    (fp_text reference D3 (at -7.048 -2.667) (layer F.SilkS))
    (fp_text value 1N5820 (at 0.508 -0.762) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -7.62 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C1-Pad1)"))
    (pad 2 thru_hole rect (at 7.62 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(D1-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 5389147B)
    (at 195.453 80.264 270)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U14 (at -10.033 5.461 360) (layer F.SilkS))
    (fp_text value 74ACT05 (at 1.27 1.27 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /emu/SEEK_DONE))
    (pad 2 thru_hole circle (at -5.08 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J2-Pad8)"))
    (pad 3 thru_hole circle (at -2.54 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /emu/WFAULT))
    (pad 4 thru_hole circle (at 0 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J2-Pad12)"))
    (pad 5 thru_hole circle (at 2.54 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /emu/SELECTED))
    (pad 6 thru_hole circle (at 5.08 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(J1-Pad1)"))
    (pad 7 thru_hole circle (at 7.62 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J2-Pad22)"))
    (pad 9 thru_hole circle (at 5.08 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /emu/READY))
    (pad 10 thru_hole circle (at 2.54 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J2-Pad20)"))
    (pad 11 thru_hole circle (at 0 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /emu/INDEX))
    (pad 12 thru_hole circle (at -2.54 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(J2-Pad10)"))
    (pad 13 thru_hole circle (at -5.08 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /emu/TRACK0))
    (pad 14 thru_hole circle (at -7.62 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Sockets_DIP.3dshapes/DIP-14__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 556D0E10)
    (at 140.843 121.92)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U15 (at -11.176 -4.699 90) (layer F.SilkS))
    (fp_text value 74ACT05 (at 1.27 1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /emu/WRITE))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(P1-Pad1)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /emu/HEAD2))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J4-Pad4)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /emu/HEAD0))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J4-Pad14)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J4-Pad18)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /emu/HEAD1))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 RECOVERY_DRIVE2_SEL))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /emu/RECOVERY))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J4-Pad2)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /emu/HEAD3))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Sockets_DIP.3dshapes/DIP-14__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-14__300 (layer F.Cu) (tedit 556D0DED)
    (at 168.021 121.92)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U16 (at -11.43 -4.572 90) (layer F.SilkS))
    (fp_text value 74ACT05 (at 3.048 -0.254) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /emu/STEP))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J4-Pad24)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 SEL2))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J4-Pad28)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /emu/SEL4))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J4-Pad32)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J4-Pad34)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /emu/DIR_IN))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J4-Pad30)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /emu/SEL3))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(J4-Pad26)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /emu/SEL1))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Sockets_DIP.3dshapes/DIP-14__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 558E08A4)
    (at 131.699 136.652 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at -4.572 0 270) (layer F.SilkS))
    (fp_text value CONN_1X2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J4-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-20__300 (layer F.Cu) (tedit 536EE181)
    (at 208.407 71.882 270)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U2 (at -13.97 4.445 360) (layer F.SilkS))
    (fp_text value 74LVC245 (at 6.35 1.27 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -11.43 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole circle (at -8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /emu/HEAD3))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /emu/HEAD2))
    (pad 4 thru_hole circle (at -3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /emu/WRITE))
    (pad 5 thru_hole circle (at -1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /emu/HEAD0))
    (pad 6 thru_hole circle (at 1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /emu/HEAD1))
    (pad 7 thru_hole circle (at 3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /emu/STEP))
    (pad 8 thru_hole circle (at 6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /emu/DIR_IN))
    (pad 9 thru_hole circle (at 8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /emu/SEL1))
    (pad 10 thru_hole circle (at 11.43 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 11 thru_hole circle (at 11.43 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 /emu/INT_SEL1))
    (pad 12 thru_hole circle (at 8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /emu/E_DIR_IN))
    (pad 13 thru_hole circle (at 6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /emu/E_STEP))
    (pad 14 thru_hole circle (at 3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /emu/E_HEAD1))
    (pad 15 thru_hole circle (at 1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /emu/E_HEAD0))
    (pad 16 thru_hole circle (at -1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /emu/E_WRITE))
    (pad 17 thru_hole circle (at -3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /emu/E_HEAD2))
    (pad 18 thru_hole circle (at -6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /emu/E_HEAD3))
    (pad 19 thru_hole circle (at -8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /emu/~EMU_EN))
    (pad 20 thru_hole circle (at -11.43 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (model Sockets_DIP.3dshapes/DIP-20__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_DIP:DIP-8__300 (layer F.Cu) (tedit 55B56166)
    (at 172.339 74.422)
    (descr "8 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U11 (at -6.1468 -4.4577 90) (layer F.SilkS))
    (fp_text value 24C256W (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(P4-Pad2)"))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(P4-Pad4)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 I2C2_SDA))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 I2C2_SCL))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 558E09E2)
    (at 214.757 26.67)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at -3.175 0) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J5-Pad4)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 558E09E9)
    (at 215.138 42.672)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at -0.08128 -2.58064) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(D1-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 558E0A1F)
    (at 125.095 51.435)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P6 (at -0.127 2.667) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 558E09CA)
    (at 191.897 96.012)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P5 (at -0.127 2.667) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C6C08)
    (at 178.435 45.72 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference F1 (at 0.635 -3.175 90) (layer F.SilkS))
    (fp_text value 3A (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 58 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 56 "Net-(C6-Pad1)"))
    (model Discret.3dshapes/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556D0D07)
    (at 200.025 129.54)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R23 (at 0.254 -3.048) (layer F.SilkS))
    (fp_text value 100 (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 88 "Net-(J6-Pad13)"))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 89 "Net-(J6-Pad14)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5571069D)
    (at 134.747 74.676 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R22 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 98 ~MFM1_IN))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 558B5A37)
    (at 157.607 93.98 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R21 (at 0.8763 2.5654 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 49 I2C2_SDA))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 558B5A3C)
    (at 161.671 93.98 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R20 (at 2.2987 -2.794 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 48 I2C2_SCL))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C6FBA)
    (at 182.88 40.894 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R19 (at -3.937 2.413 270) (layer F.SilkS))
    (fp_text value 267 (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 95 "Net-(R19-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 539902E5)
    (at 165.735 81.534)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R18 (at -1.8415 -2.6035) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 94 "Net-(P4-Pad4)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 165.735 85.09)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R17 (at 0.0254 2.6162) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 93 "Net-(P4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 170.815 103.632 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R16 (at 0.0254 2.6162 180) (layer F.SilkS))
    (fp_text value 732 (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 97 V12_ADC))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 46 AGND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C7052)
    (at 132.08 57.15 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R14 (at 8.509 -0.762 180) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 51 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 59 "Net-(D2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C6F73)
    (at 125.73 44.45)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R12 (at -5.207 2.286) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 55 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C6F68)
    (at 139.065 44.45 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R11 (at 0.254 -2.794 180) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 54 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 55 "Net-(C4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C6FA1)
    (at 156.591 41.656 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R10 (at 2.032 2.54 270) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 53 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 54 "Net-(C3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C6F9A)
    (at 165.608 43.942)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R9 (at -4.318 2.032) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 52 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 53 "Net-(C2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C6F92)
    (at 166.18 48.9585 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R8 (at 4.636 -2.0955 180) (layer F.SilkS))
    (fp_text value 1k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 51 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 52 "Net-(C1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556D0EC0)
    (at 123.571 125.984 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R7 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 85 "Net-(J4-Pad6)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538914EE)
    (at 136.271 103.124 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R5 (at 8.382 0.254 180) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 45 /emu/~MFM_READ_EN))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556D0D03)
    (at 184.531 129.54 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at 0 3.048 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 62 "Net-(J1-Pad14)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 61 "Net-(J1-Pad13)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 136.398 98.933 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0.0254 2.6162 180) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 43 /emu/~EMU_EN))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 557106A5)
    (at 138.811 74.676 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 8.128 0.508 270) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 44 /emu/~MFM0_IN))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 538685E2)
    (at 212.979 50.038)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R15 (at 0.0254 2.6162) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 97 V12_ADC))
    (pad 2 thru_hole circle (at 5.15874 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 57 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 558B5A57)
    (at 197.485 117.475 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C18 (at 5.0292 -1.2065 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 556E5BC8)
    (at 165.227 74.422 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C17 (at -0.508 3.302 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 556D0E60)
    (at 140.335 133.096 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C16 (at 0 3.048 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 5399021C)
    (at 128.651 121.92 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C15 (at -0.0635 2.6035 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 556D0CEE)
    (at 193.802 136.398 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C14 (at 0.508 2.54 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53868C0F)
    (at 195.453 67.564 180)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C13 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 53868C0F)
    (at 208.407 55.626 180)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C12 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 556D0E40)
    (at 155.829 121.92 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C11 (at -0.254 2.54 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Capacitor4x3RM2-5_RevB (layer F.Cu) (tedit 556D0CF1)
    (at 178.054 136.144 270)
    (descr "Capacitor 4mm x 2,5mm RM 2,5mm")
    (tags "Capacitor Kondensator")
    (fp_text reference C10 (at 0 2.794 270) (layer F.SilkS))
    (fp_text value .1uF (at -1.016 3.048 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 556C6C0F)
    (at 186.817 46.228 90)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C9 (at -2.667 -3.302 90) (layer F.SilkS))
    (fp_text value "22uF 10V" (at 0 3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 5399046B)
    (at 191.897 46.228 90)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C8 (at 4.826 0 180) (layer F.SilkS))
    (fp_text value "22uF 10V" (at 0 3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 556BBBE9)
    (at 196.977 46.228 90)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C7 (at 0.508 3.81 90) (layer F.SilkS))
    (fp_text value "22uF 10V" (at 0 3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 53990335)
    (at 200.66 38.735)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C6 (at 2.794 3.683) (layer F.SilkS))
    (fp_text value "10uF 25V" (at 0 3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:LDO03 (layer F.Cu) (tedit 53922E91)
    (at 191.643 37.084)
    (fp_text reference U12 (at 3.175 -14.605) (layer F.SilkS))
    (fp_text value LDO03H (at 0 -2.794) (layer F.SilkS) hide)
    (pad 5 thru_hole oval (at -3.4036 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(R19-Pad1)"))
    (pad 4 thru_hole oval (at -1.7018 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 2 thru_hole oval (at 1.7018 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(C6-Pad1)"))
    (pad 1 thru_hole rect (at 3.4036 1.7018) (size 1.3716 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(R24-Pad2)"))
    (pad 6 thru_hole circle (at -0.0762 -12.0142) (size 1.651 1.651) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556D076F)
    (at 191.135 117.348 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at 0 -3.175 90) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 103 SEL2))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 558E0A06)
    (at 204.47 50.8 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P9 (at -4.064 0.127 360) (layer F.SilkS))
    (fp_text value CONN_1X2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(P9-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C4647)
    (at 203.835 29.464 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R24 (at 5.08 2.54 90) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 104 "Net-(R24-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 556C465A)
    (at 198.755 29.464 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R25 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value 51.1k (at 3.81 3.81 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 104 "Net-(R24-Pad2)"))
    (pad 2 thru_hole circle (at 5.15874 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 1 +5V))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 557E2E06)
    (at 146.939 54.864 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R26 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value 10k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 105 "Net-(R26-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 57 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 557E2DFE)
    (at 146.939 51.054 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R27 (at -0.254 2.54 180) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 105 "Net-(R26-Pad1)"))
    (pad 2 thru_hole circle (at 5.15874 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 47 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:DIP-14__300 (layer F.Cu) (tedit 556D08A5)
    (at 209.55 117.475)
    (descr "14 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U17 (at -11.43 -5.08 90) (layer F.SilkS))
    (fp_text value 74ACT05 (at 1.27 1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(R26-Pad1)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(R26-Pad1)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 107 POWER_BUTTON))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(R6-Pad2)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 INT_SEL2))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 SEL2))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(R6-Pad2)"))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Sockets_DIP.3dshapes/DIP-14__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:screw-6-32 (layer B.Cu) (tedit 556C6E34)
    (at 191.135 18.161)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH4 (at 5.969 1.397) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -5.99948) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 0.254) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask B.SilkS))
  )
  (module all_fp:screw-6-32 (layer B.Cu) (tedit 556C6E34)
    (at 191.135 157.861)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH2 (at 5.969 1.397) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -5.99948) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 0.254) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask B.SilkS))
  )
  (module all_fp:screw-6-32 (layer F.Cu) (tedit 556C6E34)
    (at 111.887 158.115)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH3 (at 5.969 -1.397) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.99948) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 -0.254) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
  )
  (module all_fp:screw-6-32 (layer F.Cu) (tedit 556C6E34)
    (at 111.887 18.415)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH1 (at 5.969 -1.397) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.99948) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 10.287 -0.254) (size 4.7498 4.7498) (drill 3.9878) (layers *.Cu *.Mask F.SilkS))
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 558E09F7)
    (at 194.183 60.452)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P10 (at -0.127 2.667) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 558E09D3)
    (at 170.815 93.98)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference P11 (at -0.127 2.667) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.0668) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 558B5A47)
    (at 194.183 117.348 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R6 (at -8.001 -0.0254 90) (layer F.SilkS))
    (fp_text value 5.11k (at 3.81 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.00126 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 5.15874 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.SilkS *.Mask)
      (net 108 "Net-(R6-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 556FB600)
    (at 179.197 28.448 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C1 (at 4.064 5.858 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 -1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 4.5 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 4.5 -2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C1-Pad2)"))
    (pad 1 connect rect (at 2.29616 2.48488 90) (size 3.2 1.778) (layers *.Cu)
      (net 51 "Net-(C1-Pad1)"))
    (pad 2 connect rect (at 2.22504 -2.55448 90) (size 3.5 1.778) (layers *.Cu)
      (net 52 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L21_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 556FB600)
    (at 165.227 28.448 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C2 (at 4.064 5.858 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 -1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 4.5 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 0 -2.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 4.5 -2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C2-Pad2)"))
    (pad 1 connect rect (at 2.29616 2.48488 90) (size 3.2 1.778) (layers *.Cu)
      (net 52 "Net-(C1-Pad2)"))
    (pad 2 connect rect (at 2.22504 -2.55448 90) (size 3.5 1.778) (layers *.Cu)
      (net 53 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L21_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 556FB600)
    (at 137.287 28.448 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C4 (at 4.064 5.858 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 -1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 4.5 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -2.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C4-Pad2)"))
    (pad 1 thru_hole rect (at 0 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 4.5 -2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C4-Pad2)"))
    (pad 1 connect rect (at 2.29616 2.48488 90) (size 3.2 1.778) (layers *.Cu)
      (net 54 "Net-(C3-Pad2)"))
    (pad 2 connect rect (at 2.22504 -2.55448 90) (size 3.5 1.778) (layers *.Cu)
      (net 55 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L21_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 556FB600)
    (at 151.257 28.448 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C3 (at 4.064 5.858 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 -1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 4.5 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -2.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C3-Pad2)"))
    (pad 1 thru_hole rect (at 0 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 4.5 -2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C3-Pad2)"))
    (pad 1 connect rect (at 2.29616 2.48488 90) (size 3.2 1.778) (layers *.Cu)
      (net 53 "Net-(C2-Pad2)"))
    (pad 2 connect rect (at 2.22504 -2.55448 90) (size 3.5 1.778) (layers *.Cu)
      (net 54 "Net-(C3-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L21_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:CP_8x21mm (layer F.Cu) (tedit 556FB600)
    (at 123.317 28.448 90)
    (descr "Capacitor, pol, cyl 8x21mm")
    (fp_text reference C5 (at 4.064 5.858 90) (layer F.SilkS))
    (fp_text value "3F 2.7V" (at -9.144 -1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 4.5 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 0 -2.524 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 1 thru_hole rect (at 0 2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 4.5 -2.5 90) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 1 connect rect (at 2.29616 2.48488 90) (size 3.2 1.778) (layers *.Cu)
      (net 55 "Net-(C4-Pad2)"))
    (pad 2 connect rect (at 2.22504 -2.55448 90) (size 3.5 1.778) (layers *.Cu)
      (net 47 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L21_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 557C5512)
    (at 174.371 37.592 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U6 (at 2.54 4.064 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C1-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C1-Pad1)"))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44ABC)
    (at 164.719 37.592 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U7 (at 0.4445 5.08 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C2-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C1-Pad2)"))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44ABC)
    (at 136.779 38.1 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U9 (at 0.4445 5.08 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C4-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C3-Pad2)"))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:TO-92-Free-inline-wide (layer F.Cu) (tedit 53A44ABC)
    (at 125.095 38.1 270)
    (descr "TO-92 allgemein free inline wide drill 0,8mm")
    (tags "TO-92 allgemein free inline wide drill 0,8mm")
    (fp_text reference U10 (at 0.4445 5.08 270) (layer F.SilkS))
    (fp_text value KA431A (at 0.635 5.3975 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C4-Pad2)"))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module all_fp:cnp_7x4.5mm (layer F.Cu) (tedit 0)
    (at 181.356 73.6473 270)
    (descr "Capacitor non pol, 7x4,5mm")
    (fp_text reference C19 (at -0.0254 -3.5052 270) (layer F.SilkS))
    (fp_text value "22uF 10V" (at 0 3.556 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 +3V3))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text CAPS (at 202.819 54.864) (layer F.SilkS))
  (gr_text "MFM Rev B   www.pdp8online.com/mfm" (at 158.623 18.288) (layer F.SilkS))
  (gr_text WRITE (at 128.778 136.144 90) (layer F.SilkS))
  (gr_text "   DRIVE\n2   SEL   1" (at 204.2414 91.3638) (layer F.SilkS))
  (gr_text 4 (at 210.439 103.124) (layer F.SilkS))
  (gr_text 1 (at 210.439 95.504) (layer F.SilkS))
  (gr_text 3.3V (at 171.323 90.932) (layer F.SilkS))
  (gr_text 5V (at 197.739 60.452) (layer F.SilkS))
  (gr_text 3 (at 178.1175 87.503) (layer F.SilkS))
  (gr_text 1 (at 175.387 87.503) (layer F.SilkS))
  (gr_text 34 (at 222.1992 104.3559 90) (layer B.SilkS))
  (gr_text 2 (at 222.25 63.8048 90) (layer B.SilkS))
  (gr_text 20 (at 222.4659 149.4663 90) (layer B.SilkS))
  (gr_text 2 (at 222.2754 126.9873 90) (layer B.SilkS))
  (gr_text 1 (at 207.264 128.27 90) (layer F.SilkS))
  (gr_text 20 (at 218.44 152.908 90) (layer F.SilkS))
  (gr_text 20 (at 153.5303 98.7679 90) (layer F.SilkS))
  (gr_text 1 (at 142.24 74.168 90) (layer F.SilkS))
  (gr_text 20 (at 200.787 142.875) (layer F.SilkS))
  (gr_text 1 (at 178.308 153.924) (layer F.SilkS))
  (gr_text 34 (at 166.7256 142.9131) (layer F.SilkS))
  (gr_text 1 (at 125.73 153.924) (layer F.SilkS))
  (gr_line (start 128.143 93.98) (end 117.475 93.98) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 128.143 76.2) (end 128.143 93.98) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 117.475 76.2) (end 128.143 76.2) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 117.475 76.2) (end 117.475 14.986) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 117.475 161.036) (end 117.475 93.98) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_text GND (at 125.095 48.768) (layer F.SilkS))
  (gr_text GND (at 187.833 96.012) (layer F.SilkS))
  (gr_line (start 222.885 130.937) (end 222.885 130.175) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 222.885 68.072) (end 222.885 67.31) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 14.986) (end 224.155 14.986) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 52.578) (end 234.315 14.986) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 52.578) (end 234.315 52.578) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 61.595) (end 224.155 52.578) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 61.595) (end 224.155 61.595) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 62.357) (end 233.553 61.595) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 67.31) (end 234.315 62.357) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 222.885 67.31) (end 234.315 67.31) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 68.072) (end 222.885 68.072) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 106.045) (end 234.315 68.072) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 106.807) (end 234.315 106.045) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 106.807) (end 233.553 106.807) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 124.46) (end 224.155 106.807) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 124.46) (end 224.155 124.46) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.68 124.587) (end 233.553 124.46) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 125.222) (end 233.68 124.587) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 130.175) (end 234.315 125.222) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 222.885 130.937) (end 234.315 130.937) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 130.175) (end 222.885 130.175) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 234.315 151.13) (end 234.315 130.937) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 233.553 151.892) (end 234.315 151.13) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 232.791 151.892) (end 233.553 151.892) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 151.892) (end 232.791 151.892) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 224.155 161.036) (end 224.155 151.892) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_text 12V (at 215.138 45.72) (layer F.SilkS))
  (gr_text 5V (at 215.138 23.749) (layer F.SilkS))
  (gr_line (start 117.475 161.036) (end 224.155 161.036) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 224.155 14.986) (end 117.475 14.986) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.569 106.807) (xy 223.901 106.807) (xy 223.901 61.595) (xy 234.569 61.595)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.901 61.595) (xy 223.901 106.807) (xy 234.569 106.807) (xy 234.569 61.595) (xy 223.9645 61.595)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.569 151.892) (xy 223.901 151.892) (xy 223.901 124.46) (xy 234.569 124.46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.00254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.569 151.892) (xy 223.901 151.892) (xy 223.901 124.46) (xy 234.569 124.46)
      )
    )
  )
  (zone (net 47) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.187 50.8) (xy 222.123 50.8) (xy 222.123 156.464) (xy 118.999 156.464) (xy 118.999 95.504)
        (xy 129.667 95.504) (xy 129.667 74.676) (xy 118.999 74.676) (xy 118.999 20.32) (xy 226.187 20.32)
      )
    )
  )
  (zone (net 47) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.187 50.8) (xy 222.123 50.8) (xy 222.123 156.464) (xy 118.999 156.464) (xy 118.999 95.504)
        (xy 129.667 95.504) (xy 129.667 74.676) (xy 118.999 74.676) (xy 118.999 20.32) (xy 226.187 20.32)
      )
    )
  )
)
