(footprint "Pin_Header_Straight_2x10" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "1 pin")
  (tags "CONN DEV")
  (property "Sheetfile" "emu.kicad_sch")
  (property "Sheetname" "emu")
  (attr through_hole)
  (fp_text reference "J3" (at -1.651 5.588) (layer "F.SilkS"))
  (fp_text value "CON20" (at 0 0) (layer "F.SilkS") hide)
  (pad "1" thru_hole rect (at -11.43 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "2" thru_hole oval (at -11.43 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "3" thru_hole oval (at -8.89 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "4" thru_hole oval (at -8.89 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "5" thru_hole oval (at -6.35 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "6" thru_hole oval (at -6.35 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "7" thru_hole oval (at -3.81 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "8" thru_hole oval (at -3.81 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "9" thru_hole oval (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "10" thru_hole oval (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "11" thru_hole oval (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "12" thru_hole oval (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "13" thru_hole oval (at 3.81 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "14" thru_hole oval (at 3.81 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "15" thru_hole oval (at 6.35 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "16" thru_hole oval (at 6.35 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "17" thru_hole oval (at 8.89 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "18" thru_hole oval (at 8.89 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "19" thru_hole oval (at 11.43 1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (pad "20" thru_hole oval (at 11.43 -1.27) (size 1.7272 1.7272) (drill 1.0668) (layers "*.Cu" "*.Mask" "F.SilkS"))
  (model "Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
